Patch-ID# 113616-04
Keywords: ultra5 ultra10 ultra30 ultra60 sunblade ideas sunpci cadence java plug-in lo0 keyboard staroffice mouse sunray ipv6
Synopsis: SunPCi2 2.3.2: for Solaris 7, 8, 9 and sparc architectures
Date: Aug/13/2003


Install Requirements: None                      
                      
Solaris Release: 7 8 9

SunOS Release: 5.7 5.8 5.9

Unbundled Product: SunPCI

Unbundled Release: 2.3.2

Xref: 

Topic: 

Relevant Architectures: sparc

BugId's fixed with this patch: 4759220 4762057 4784924 4799283 4802253 4806545 4808623 4825915 4835567 4901949

Changes incorporated in this version: 4901949

Patches accumulated and obsoleted by this patch: 

Patches which conflict with this patch: 

Patches required with this patch: 

Obsoleted by: 

Files included with this patch: 

/opt/SUNWspci2/bin/get_nvl_interface
/opt/SUNWspci2/bin/sparcv9/sunpcbinary
/opt/SUNWspci2/bin/sunpcbinary
/opt/SUNWspci2/bin/sunpci
/opt/SUNWspci2/bios/bios.bin
/opt/SUNWspci2/drivers/solaris/sunpcidrv.270
/opt/SUNWspci2/drivers/solaris/sunpcidrv.270.64
/opt/SUNWspci2/drivers/solaris/sunpcidrv.280
/opt/SUNWspci2/drivers/solaris/sunpcidrv.280.64
/opt/SUNWspci2/drivers/solaris/sunpcidrv.290
/opt/SUNWspci2/drivers/solaris/sunpcidrv.290.64
/opt/SUNWspci2/drivers/solaris/sunpcidrv.conf
/opt/SUNWspci2/drivers/solaris/sunpcload
/opt/SUNWspci2/drivers/win2k/symbols/sunvideo.pdb
/opt/SUNWspci2/drivers/winnt/patch/sunvideo/win2k/sunvideo.dll
/opt/SUNWspci2/drivers/winnt/patch/sunvideo/winxp/sunvideo.dll
/opt/SUNWspci2/drivers/winnt/patch/system/win2k/sunnpdll.dll
/opt/SUNWspci2/drivers/winnt/patch/system/winxp/sunnpdll.dll
/opt/SUNWspci2/drivers/winxp/symbols/sunvideo.pdb

Problem Description:

Note:
        Other fixes added to this patch

        Some menus have incorrect default path

        Fix to disallow booting SunPCi3 images with a SunPCi2 board

        Network provider fix

        Copy and paste fix

        Mouse fixes

        sunpci2test no longer hangs on a Rev -03 SunPCi-2 card.

        Fixed "Warning!! Your CPU has been changed" in BIOS 1.017


4901949  Virtual networking errors when IPv6 is enabled


(113616-03)

4825915  USB keyboard mapping problem
4806545  Delay when paging or scrolling through docs in staroffice
4835567  SUNVTS test reports error while waking up "OFF" SUNPCI card
4799283  pci108e, 7063 PM: lots of errors with cycle test


(113616-02)

4808623  Right mouse click not working when xdisplaying to sunray appliance


(113616-01)

4759220  Colormap for IDEAS menu bar remains solid black when SunPCi window is active.
4762057  Cadence application crash
4802253  Java Plug-in 1.3.1_06 is blank
4784924  SunPCi selects lo0 as the default interface in some cases

Patch Installation Instructions:
-------------------------------- 
For Solaris 7-9 releases, refer to the man pages for instructions
on using 'patchadd' and 'patchrm' scripts provided with Solaris.
Any other special or non-generic installation instructions should be
described below as special instructions.  The following example
installs a patch to a standalone machine:
 
        example# patchadd /var/spool/patch/104945-02
 
The following example removes a patch from a standalone system:
 
        example# patchrm 104945-02
 
For additional examples please see the appropriate man pages.

Special Install Instructions:
----------------------------- 
After applying this patch, run:
 
Change to superuser
cd /opt/SUNWspci2/drivers/solaris
./sunpcload
 
Flashing the bios to 1.017:
cd /opt/SUNWspci2/drivers/solaris
./sunpciflash -f /opt/SUNWspci2/bios/bios.bin
 
Updating the intel drivers:(See the 2.3.2 release notes for more detailed instructions)
 
Launch Microsoft Windows 
 
*For Windows XP, 2000 Pro, NT4 Workstation users*
Windows will recognize the patch is installed and update the intel drivers
automatically after loggin in.  Users only needs to click the "OK" button on the screen
stating, "Would you like to update your intel drivers", and restart Windows when
prompted.  
 
*For Windows Server products, 98SE, and manually updating drivers*
Follow the steps below for the appropiate Operating System if any of the following criteria 
exists, or if the auto update program fails:
	auto update program fails with message about "drivers already updated"
	Windows Server product installed
	Windows 98SE is installed
 
For Windows 98SE users:
 
    Run F:\drivers\win98\setup.exe 
    Select "update my drivers", and follow the instructions 
 
For Windows Server products
    1. Disconnect all clients and log in as administrator
    2. Run c:\SUN\SUNFSD\FSDON.REG
    3. Follow steps 1-3 below for the appropiate Windows product 
    4. Run c:\SUN\SUNFSD\FSDOFF.REG   
 
For Windows NT Users:(IF auto update drivers program fails)
*If auto update fails with message "drivers already updated", click cancel and run
the following command at a dos box before preceding: c:\sun\tools\verchk.exe -invalidate
    1. Map a drive to \\localhost\opt\SUNWspci2
    2. Using the drive letter mapped above, traverse to the directory \drivers\winnt\patch
    3. Double-click update.bat, and follow the instructions.
 
For Windows 2000 Users:(If auto update drivers program fails)
*If auto update fails with message "drivers already updated", click cancel and run
the following command at a dos box before preceding: c:\sun\tools\verchk.exe -invalidate
    1. Map a drive to \\localhost\opt\SUNWspci2
    2. Using the drive letter mapped above, traverse to the directory \drivers\win2k\patch
    3. Double-click update.bat, and follow the instructions.
 
For Windows XP Users:(If auto update drivers program fails)
*If auto update fails with message "drivers already updated", click cancel and run
the following command at a dos box before preceding: c:\sun\tools\verchk.exe -invalidate
    1. Map a drive to \\localhost\opt\SUNWspci2
    2. Using the drive letter mapped above, traverse to the directory \drivers\winxp\patch
    3. Double-click udate.bat, and follow the instructions
-----------------------------

README -- Last modified date:  Wednesday, August 13, 2003

