This function can be used to:
- Generate a list of required patches for a storage system.
- Install these patches on each component of the storage system.
NOTE: Selecting a device will install all patches listed for that device. The Service processor does not allow selection of individual patches.
WARNING: For array upgrades, you must ensure the array is redundant prior to performing the upgrade operation or temporary loss of data availability can occur. Disk drive upgrades require ALL I/O to the array be quiesced. Turn-off device monitoring to avoid false events during upgrade.