## Device Discovery Page

Field | Description
Agents running | Displays how many agents are currently running.
Agents done | Displays how many agents have completed the discovery run.
Devices found | Click to display details about the discovered devices in a pop-up window. The results show the following: Agent Type-device type Name IP-IP address of the device Comments
Host | Select a host from the pull-down menu from which the agents will run.
Product/Discovery Method | Select a product or a discovery method from the following list: Devices from IP List (the default)-All devices that have been entered in the `/etc/deviceIP.conf` file are discovered. Depending on the size of the monitored configuration, this process might take a few minutes. Note: JOBOD devices cannot be discovered using the Devices from IP List method. Inband discovery-In-band devices, including internal disks, Sun StorEdge A5x00 arrays, and tape devices are discovered. Inband Sun 3120JBOD/3310JBOD/3310/3510/3511 Discovery - Includes: StorEdge 3120 SCSI array (JBOD) Sun StorEdge 3310 SCSI array (RAID Controller) Sun StorEdge 3310-D SCSI array (JBOD) Sun StorEdge 3510 FC array (RAID Controller) Sun StorEdge 3511 FC array (RAID-SATA Controller) Sun StorEdge 5210 Array Sun StorEdge A3500FC array Sun StorEdge D2 array Subnet-uses SNMP to query and discover supported switches and arrays. such as the Sun StorEdge 9900 Series systems,.
| Click to activate Discovery.