MQ Queue Name     (Overview)

DESCRIPTION
This datapoint is the name of the MQSeries Queue that can be
accessed from a Sun MTP transaction via the Sun MTP MQSeries 
server when MQSeries messaging and queuing services are available.

The Sun MTP MQSeries server, unikixqm, must be active for any application 
using the MQSeries API.  The unikixqm server may be enabled through the 
-q option when starting the Sun MTP server unikixmain. The Sun MTP Transaction 
server, unikixtran must also be rebuilt to support MQSeries access.


VALUES
"MQ Queue Name" consists of 1-40 characters.
Note that this datapoint is set to "N/A" when the MQSeries messaging  
and queuing services are not available and the "MQ Available" datapoint 
displays a value of "No". 


INTERPRETATION
This datapoint, along with the MQ Queue Manager value are sufficient to 
identify the MQSeries Queue that is being monitored by the current Sun MTP
System when MQSeries services are available.

