FS Out            (DCT Remote)

DESCRIPTION 
"FS Out" shows the number of outbound Function Ship (FS) requests for a given
transient data queue (TD).


VALUES
The value of "FS Out" is a number representing a request count.


INTERPRETATION
Sun MTP processes an FS out under two circumstances. First, a local application
program may issue a READQ TD or WRITEQ TD against a remote TD queue. Sun MTP 
ships the request to the system identified by "RSys" for the queue called 
"RName". The other condition where this happens is by a request generated by a 
remote application program. Such a program's region could have the TD queue 
defined as residing in the Sun MTP region while the TD queue can actually reside 
somewhere else. In this case, Sun MTP forwards the request to the "RSys" that it 
knows about. Regardless of the situation, Sun MTP increments "FS Out" each time 
it processes a FS for access to a remote TD queue.


CONCLUSIONS
This datapoint can give you a general idea of the volume of data transferred to 
remote regions from the local Sun MTP system for a specific TD queue.
