Hardware Compatibility List

for Solaris 2.6 (Intel Platfor m

Edition)

Sun Microsystems, Inc.

901 San Antonio Road

Palo Alto, CA 94303

U.S.A.

Part No: 802-5739{02

January 1998

Copyright 1997 Sun Microsystems, Inc. 901 San Antonio Road, Palo Alto, California 94303-4900 U.S.A. All rights reserved.

This product or document is protected by copyright and distributed under licenses restricting its use, copying, distribution, and

decompilation. No part of this product or document may be reproduced in any form by any means without prior written

authorization of Sun and its licensors, if any. Third-party software, including font technology, is copyrighted and licensed from

Sun suppliers.

Parts of the product may be derived from Berkeley BSD systems, licensed from the University of California. UNIX is a

registered trademark in the U.S. and other countries, exclusively licensed through X/Open Company, Ltd.

Sun, Sun Microsystems, the Sun logo, SunSoft, SunDocs, SunExpress, and Solaris are trademarks, registered trademarks, or

service marks of Sun Microsystems, Inc. in the U.S. and other countries. All SPARC trademarks are used under license and are

trademarks or registered trademarks of SPARC International, Inc. in the U.S. and other countries. Products bearing SPARC

trademarks are based upon an architecture developed by Sun Microsystems, Inc.

The OPEN LOOK and Sun TM Graphical User Interface was developed by Sun Microsystems, Inc. for its users and licensees. Sun

acknowledges the pioneering efforts of Xerox in researching and developing the concept of visual or graphical user interfaces

for the computer industry. Sun holds a non-exclusive license from Xerox to the Xerox Graphical User Interface, which license

also covers Sun’s licensees who implement OPEN LOOK GUIs and otherwise comply with Sun’s written license agreements.

RESTRICTED RIGHTS: Use, duplication, or disclosure by the U.S. Government is subject to restrictions of FAR

52.227{14(g)(2)(6/87) and FAR 52.227{19(6/87), or DFAR 252.227{7015(b)(6/95) and DFAR 227.7202{3(a).

DOCUMENTATION IS PROVIDED \AS IS" AND ALL EXPRESS OR IMPLIED CONDITIONS, REPRESENTATIONS AND

WARRANTIES, INCLUDING ANY IMPLIED WARRANTY OF MERCHANTABILITY, FITNESS FOR A PARTICULAR

PURPOSE OR NON-INFRINGEMENT, ARE DISCLAIMED, EXCEPT TO THE EXTENT THAT SUCH DISCLAIMERS ARE

HELD TO BE LEGALLY INVALID.

Copyright 1997 Sun Microsystems, Inc. 901 San Antonio Road, Palo Alto, Californie 94303-4900 Etats-Unis. Tous droits rØ servØ s.

Ce produit ou document est protØ gØ par un copyright et distribuØ avec des licences qui en restreignent l’utilisation, la copie, la

distribution, et la dØ compilation. Aucune partie de ce produit ou document ne peut Œ tre reproduite sous aucune forme, par

quelque moyen que ce soit, sans l’autorisation prØ alable et Ø crite de Sun et de ses bailleurs de licence, s’il y en a. Le logiciel

dØ tenu par des tiers, et qui comprend la technologie relative aux polices de caractŁ res, est protØ gØ par un copyright et licenciØ

par des fournisseurs de Sun.

Des parties de ce produit pourront Œ tre dØ rivØ es du systŁ me Berkeley BSD licenciØ s par l’UniversitØ de Californie. UNIX est une

marque dØ posØ e aux Etats-Unis et dans d’autres pays et licenciØ e exclusivement par X/Open Company, Ltd.

Sun, Sun Microsystems, le logo Sun, SunSoft, SunDocs, SunExpress, et Solaris sont des marques de fabrique ou des marques

dØ posØ es, ou marques de service, de Sun Microsystems, Inc. aux Etats-Unis et dans d’autres pays. Toutes les marques SPARC

sont utilisØ es sous licence et sont des marques de fabrique ou des marques dØ posØ es de SPARC International, Inc. aux

Etats-Unis et dans d’autres pays. Les produits portant les marques SPARC sont basØ s sur une architecture dØ veloppØ e par Sun

Microsystems, Inc.

L’interface d’utilisation graphique OPEN LOOK et Sun TM a Ø tØ dØ veloppØ e par Sun Microsystems, Inc. pour ses utilisateurs et

licenciØ s. Sun reconna� ^ t les efforts de pionniers de Xerox pour la recherche et le dØ veloppement du concept des interfaces

d’utilisation visuelle ou graphique pour l’industrie de l’informatique. Sun dØ tient une licence non exclusive de Xerox sur

l’interface d’utilisation graphique Xerox, cette licence couvrant Ø galement les licenciØ s de Sun qui mettent en place l’interface

d’utilisation graphique OPEN LOOK et qui en outre se conforment aux licences Ø crites de Sun.

CETTE PUBLICATION EST FOURNIE \EN L’ETAT" ET AUCUNE GARANTIE, EXPRESSE OU IMPLICITE, N’EST

ACCORDEE, Y COMPRIS DES GARANTIES CONCERNANT LA VALEUR MARCHANDE, L’APTITUDE DE LA

PUBLICATION A REPONDRE A UNE UTILISATION PARTICULIERE, OU LE FAIT QU’ELLE NE SOIT PAS

CONTREFAISANTE DE PRODUIT DE TIERS. CE DENI DE GARANTIE NE S’APPLIQUERAIT PAS, DANS LA MESURE OU

IL SERAIT TENU JURIDIQUEMENT NUL ET NON AVENU.

Contents 1.

Hardware Compatibility List for Solaris 2.6 (Intel Platform Edition) 1How

This Document Is Organized 2

Conventions Used 3

How to Obtain Updated Hardware Compatibility Lists and Device

Driver Information 4

Related Documentation Only 4

Related Books 5

Ordering Sun Documents 5

Corrections and Additions 5

Accessing Sun Documentation Online 6

How to Obtain T echnical Support 6

General Requirements 7

System Platforms 7

Notebook Computers Certi�ed After March 1996 46

Supported Devices 48Contents iii

ivHardware

Compatibility List for Solaris 2.6 (Intel Platform Edition)¤ January 1998

CHAPTER

1 Hardware

Compatibility List for

Solaris 2.6 (Intel Platform Edition) This document provides information about general x86 hardware

requirements and the peripherals and system platforms that are supported in

the SolarisTM 2.6Intel Platform Edition computing environment.

Throughout the Solaris 2.6 release cycle, support for additional systems will

be added to the product on an ongoing basis. This document will continue to

be updated to describe the new support. Y ou can access the locations listed

in \How to Obtain Updated Hardware Compatibility Lists and Device Driver

Information" on page 4 to see if a more current version exists. Note

- The term \x86" refers to the Intel 8086 family of microprocessor

chips, including the Pentium, Pentium Pro, and Pentium IIprocessors and

compatible microprocessor chips made by AMD and Cyrix. In this document

the term \x86" refers to the overall platform architecture, whereas \Intel

Platform Edition" appears in the product name.

System platforms listed in this document are tested \as-shipped" by the

hardware manufacturers. Since it is the nature of this industry to have

unexpected and unannounced changes, SunSoft is committed to working

with customers who experience dif�culties installing the Solaris software on

supported systems. If any problems are encountered with this release,

contact your Sun Software Support Provider (SSSP). In North America, you

can also call SunSoft T echnical Support at 1-800-SUNSOFT, option 4.1

Note

-It is common practice for hardware vendors to release variants of a

particular hardware design under a single marketing name. In some cases,

not all variants will work with the current Solaris device driver. CheckDriver

Update Guide for Solaris 2.6 (Intel Platform Edition) and Device Reference

Pages for Solaris 2.6 (Intel Platform Edition) to see if they provide additional

information about speci�c hardware versions supported by the current

Solaris device driver. How

This Document Is Organized

This document is divided into these major sections:�

\General Requirements " on page 7 lists the x86 hardware requirements

for installing the Solaris 2.6 operating environment.

� \System Platforms" on page 7 lists the platforms supported in the Solaris

2.6 Intel Platform Edition product; not all of the peripherals listed in

\Supported Devices" on page 48 have been tested in all combinations on

all of these platforms. This is not intended to be an exhaustive list of x86

machines that can run Solaris 2.6 software.

� \Supported Devices" on page 48 lists the supported peripherals.

Speci�c machines and classes of devices are shown in these tables in this

document.

� \System Platforms" on page 7

� Single Processor Systems, T able 1{1

� Multiprocessor Systems (SMP), T able 1{2

� Notebook Computers (Prior to March 1996), T able 1{3

� Notebook Certi�cation Matrix (After March 1996), T able 1{4

� \Supported Devices" on page 48

� SCSI Host Bus Adapters, T able 1{5

� SCSI RAID Controllers, T able 1{6

� Solid State SCSI Disk Devices, T able 1{7

� CD-ROM Drives, T able 1{8

� Printing Devices, T able 1{9

� Audio Devices, T able 1{10

� T elephony Products, T able 1{112

Hardware

Compatibility List for Solaris 2.6 (Intel Platform Edition)¤ January 1998

�Multiport

Serial Adapters, T able 1{12

� Network Adapters|Ethernet, T able 1{13

� Network Adapters|Fast Ethernet, T able 1{14

� Network Adapters|T oken Ring, T able 1{15

� Network Adapters|W AN, T able 1{16

� AT-ISDN Adapters, T able 1{17

� High-Speed Networking, T able 1{18

� PC Card (PCMCIA)|Add-On Boards, T able 1{19

� PC Card (PCMCIA)|GPS and Navigation Devices, T able 1{20

� PC Card (PCMCIA)|Modems, T able 1{21

� PC Card (PCMCIA)|Serial Cards, T able 1{22

� PC Card (PCMCIA)|SRAM Memory Cards, T able 1{23

� Pointing Devices, T able 1{24

� T ape Drives|SCSI, T able 1{25

� SCSI RAID T ape, T able 1{26

� Uninterruptable Power Supplies (UPS), T able 1{27

� Motherboards, T able 1{28

� Video Display Adapters, T able 1{29

� Notebook Display Video Support, T able 1{30 Conventions

Used

� Pentium system platforms and motherboards listed in this document show

the CPU type and speed in parentheses after the model name.�

The term (P-xxx) indicates a Pentium processor; the xxx is replaced by the speed

of the system in megahertz. For example, P-100 indicates a 100-MHz Pentium

processor.

� The term (PP-xxx) indicates a Pentium Pro processor; the xxx is replaced by the

speed of the system in megahertz. For example, PP-150 indicates a 150-MHz

Pentium Pro processor.

� The term (PII-xxx) indicates a Pentium II processor; the xxx is replaced by the

speed of the system in megahertz. For example, PII-233 indicates a 233-MHz

Pentium II processor.Hardware Compatibility List for Solaris 2.6 (Intel Platform Edition)3

�In \Supported Devices" on page 48, peripherals that require additional

con�guration and that have a Device Reference Page inDevice Reference

Pages for Solaris 2.6 (Intel Platform Edition) are marked with a # symbol.

� Entries marked with an asterisk (*) are newly supported and require a

Driver Update for proper operation. How to Obtain Updated Hardware

Compatibility Lists and Device

Driver Information

Hardware Compatibility Lists and Driver Update releases (including related

documentation) are produced periodically as support for new hardware

becomes available. They are available from these sources:

� The W eb|For Driver Updates, open URLhttp://access1.sun.com/drivers/.For updated Hardware

Compatibility Lists, open URL

http://access1.sun.com/certify/hcl.html.

� FTP|Use anonymous FTP to access ftp://ftp.uu.net (or open URL

ftp://ftp.uu.net), then go to /vendor/sun/solaris/x86/du/ for

Driver Updates or to /vendor/sun/solaris/x86/hcl/ for Hardware

Compatibility Lists.

� CompuServe|T ype go sunsoft and go to the Solaris x86 library .

Note that the W eb, CompuServe, and ASK-IT (below) also point to

Support-provided installation and con�guration information as well as

answers to frequently asked questions.Related

Documentation Only

� Email Autoresponder|T o obtain a Hardware Compatibility List or a

Driver Update Announcement via email, write to hcl-index@sun.com

for a list of autoresponse aliases that return hardware support information.

� ASK-IT 1 |SunSoft’s Automated Support Fax-on-Demand Service�

In North America, call one of these numbers:

1-800-SUNSOFT and choose options 4, 1, 1, 1

1. Includes the current Hardware Compatibility List and document No. 51251, which summarizes the

current Driver Update.4

Hardware

Compatibility List for Solaris 2.6 (Intel Platform Edition)¤ January 1998

(310)

348-6219 and choose option 1�

Outside North America, call one of these numbers and choose option 1:

Australia 61-2-844-5374

Japan 03-5717-2560

Singapore 65-383-1971

United Kingdom 44-1276-677131 Related

Books

For speci�c hardware con�guration information necessary to install and run

the Solaris environment on your particular hardware, see the Con�guring

Devices module in the Information Library and any documentation supplied

with a Solaris 2.6Intel Platform Edition Driver Update.

Ordering Sun Documents

The SunDocs SM program provides over 250 manuals from Sun Microsystems,

Inc. If you live in the U.S., Canada, Europe, or Japan, you can purchase

documentation sets or individual manuals using this program.

For a list of documents and ordering information, see the catalog section of

SunExpressTM On The Internet athttp://www.sun.com/sunexpress.

Corrections and Additions

V endors, OEMs, and manufacturers: T o supply corrections or add products to

this list, or to obtain information on the hardware certi�cation program, send

email to x86-certify@cypress.west.sun.com or leave voice mail at

(310) 348-6170.

Hardware Compatibility List for Solaris 2.6 (Intel Platform Edition)5

Accessing Sun Documentation

Online The docs.sun.com W eb site enables you to access Sun technical

documentation online. Y ou can browse the docs.sun.com archive or search

for a speci�c book title or subject. The URL is http://docs.sun.com.

How to Obtain T echnical Support

T o obtain technical support:�

Contact your Sun Software Support Provider.

� In North America, you can also call 1-800-SUNSOFT and choose option 4.6

Hardware

Compatibility List for Solaris 2.6 (Intel Platform Edition)¤ January 1998

General Requirements CPU

Minimum

Memory Bus

Disk

Interface

Distribution

Media Devices for

Installing

Solaris Intel or compatible 386@33MHz

(minimum 1 )

Intel or compatible 486DX,

486DX2, 486SL, 486SX, 486DX4

Intel Pentium

Intel Pentium Pro

Intel Pentium II

Intel Pentium with MMX

AMD 486DX2-66

AMD 486DX2-80

AMD 486DX4-100

AMD 486DX4-100 Enhanced

AMD-K5

AMD-K6

Cyrix 486DLC-40

Cyrix 5x86-100GP

Cyrix 6x86-P120+GP

Cyrix 6x86-P150+

Cyrix 6x86MX-PR150

Cyrix 6x86-P166+ 32 Mbytes ISA,

EISA,

MCA,

PCI,

VLB IDE,

E-IDE,

SCSI CD-ROM

and a single

boot diskette Diskette driveand one of the

following

devices:

• Local SCSI

or ATAPI/IDE

CD-ROM

drive

• Remote SCSI

or ATAPI/IDE

CD-ROM

drive available

over the

network

• Remote hard

disk available

over the

network

1. A 486DX, 486DX2, or Pentium CPU is recommended for better performance.

System PlatformsSolaris

2.6Intel Platform Edition has been successfully installed and tested on

the computers listed in this section con�gured as they are shipped by the

system manufacturer.Hardware Compatibility List for Solaris 2.6 (Intel Platform Edition)7

TABLE

1{1Single Processor Systems Acer

AcerAltos 300 (P-166)

Acer AcerAltos 700

Acer AcerAltos 8001

Acer AcerAltos 800/P (P-90)

Acer AcerAltos 900 (PP-200 E-IDE)

Acer AcerAltos 900 (PP-200 SCSI)

Acer AcerAltos 7000 (P-60)

Acer AcerAltos 7000 (P-90)

Acer AcerAltos 7000/P (1 CPU, P-90)

Acer AcerAltos 9000 Pro (PP-200)

Acer AcerAltos 19000 (PP-200)

Acer AcerPower 5000 (P-60) 2 3 Acer AcerPower 5020 (P-90) 2 3 Acer AcerPower 7500 (P-75)

Acer AcerPower 9000T

Acer AcerPower Pentium P-75 Desktop

Acer AcerAltos 17000 Server (tested w/ 1 CPU only) 4 ALR BusinessVEISA DX2/66

ALR Evolution 150 (PP-150)

ALR Evolution 5DT (P-120)

ALR Evolution 5DT (P-166)

ALR Evolution Dual6 (1 CPU version, PP-200)

ALR Evolution IV 4DX2/66

ALR Evolution Q/MP2 100 (1 CPU con�g)

ALR Evolution V STe/75 (P-75)

ALR Evolution V ST/75 (P-75)

ALR Evolution V ST/120 (P-120)

ALR Evolution V ST/PCI (P-90)

ALR Evolution VQ EISA (P-60)

ALR Evolution VQ EISA (P-66)

ALR Evolution VQ EISA (P-90)8

Hardware

Compatibility List for Solaris 2.6 (Intel Platform Edition)¤ January 1998

TABLE

1{1Single Processor Systems(continued)

ALR Evolution X/75 (P-75)

ALR Evolution X/120 (P-120)

ALR FLYERvl 486 DX2/66

ALR Optima DT/133 (P-133)

ALR Optima MT (PP-200)

ALR PROVEISA DX2/66

ALR Revolution Dual6 (1 CPU con�g, PP-200, 512K)

ALR Revolution MP-100 (1 CPU con�g)

ALR Revolution MP-120 (1 CPU con�g)

ALR Revolution MP-133 (1 CPU con�g)

ALR Revolution MP-166 (1 CPU, P-166)

ALR Revolution MP II (1 CPU, P-166)

ALR Revolution MP II (1 CPU, P-200)

ALR Revolution Q-SMP (1 CPU, P-166)

ALR Revolution Quad6-200 (1 CPU, PP-200)

AMD Desktop 5K86-90 (P-90)

AMD Enhanced (486DX4-100)

American Micro Group P90PE-SS Server

American Micro Group P90PE-WS Workstation

AST Advantage Model 7302 (P-120)

AST Advantage Model 7303 (P-133)

AST Advantage Model 7304 (P-166)

AST Advantage Model 9302 (P-120)

AST Advantage Model 9304 (P-133)

AST Advantage Model 9308 (P-166)

AST Bravo LC 4/100T

AST Bravo LCP-100 (P-100)

AST Bravo MS P/75

AST Bravo MS P/75 (Eagle) (P-75)

AST Bravo MS P/75 (Monaco) (P-75)

AST Bravo MS P/90Hardware Compatibility List for Solaris 2.6 (Intel Platform Edition)9

TABLE

1{1Single Processor Systems(continued)

AST Bravo MS P/100 (P-100)

AST Bravo MS P/100 (Eagle) (P-100)

AST Bravo MS P/100 (Monaco) (P-100)

AST Bravo MS P/120 (Eagle) (P-120)

AST Bravo MS P/133 (Eagle) (P-133)

AST Bravo MS P/133 (Monaco) (P-133)

AST Bravo MS P/166 (Monaco) (P-166)

AST Bravo MS 4/50d

AST Bravo MS 4/50s

AST Bravo MS 4/66d

AST Bravo MST P100 (P-100)

AST Bravo MST P120 (Eagle) (P-120)

AST Bravo MST P133 (P-133)

AST Bravo MST 6150 (PP-150)

AST Bravo MST 6180 Model 1600C (PP-180)

AST Bravo MST 6200 Model 2500C

AST Manhattan G

AST Manhattan P5090 (P-90)

AST Manhattan P Series 5100 (P-100)

AST Manhattan P5133 12003AE (1 CPU)

AST Manhattan S6200 Model 2003 (PP-200)

AST Manhattan S6200 Model 2003LC (PP-200)

AST Manhattan V5090 (P-90)5

AST PowerExec 4/33SL

AST Premium SE 4/50

AST Premmia GX (P-90) E-IDE

AST Premmia GX (P-90) Integrated SCSI 5 AST Premmia GX (P-100)

AST Premmia GX (P-133)

AST Premmia MTE 4/6610

Hardware

Compatibility List for Solaris 2.6 (Intel Platform Edition)¤ January 1998

TABLE

1{1Single Processor Systems(continued)

AST Premmia MX 4/100t 486 DX4-100

AST Premmia MX P/75 (P-75)

AT&T GIS 3404 Server (P-90)

Austin Direct Af�nity SE

Austin Direct Power System 66 (Pentium 66)

C&S V ertriebs GmbH AMICUS Advanced (P-133)

C&S V ertriebs GmbH AMICUS Performance (P-100)

C&S V ertriebs GmbH (P-100 ISA/PCI)

Centerprise LEO-486 (486DX33)

Compaq Deskpro 4/33i

Compaq Deskpro 2000 (P-166)

Compaq Deskpro 2000 M6200 (PP-200)

Compaq Deskpro 5100 (P-150)

Compaq Deskpro 5133 (P-133)

Compaq Deskpro 5166 (P-166)

Compaq Deskpro 6000 Model 5166PDS (P-166)

Compaq Deskpro XE 450

Compaq Deskpro XE 560 (P-60)

Compaq Deskpro XL 466 (486DX2/66)

Compaq Deskpro XL 486 (486-66)

Compaq Deskpro XL 590 (P-90)

Compaq Deskpro XL 5120 (P-120)

Compaq Deskpro XL 6150 (PP-150)

Compaq Deskpro XL 6200 (PP-200)

Compaq Professional Workstation 5000 (PP-200)

Compaq ProLiant 1500 (P-75)

Compaq ProLiant 800 (PP-200)

Compaq ProLiant 850R (PP-200)Hardware Compatibility List for Solaris 2.6 (Intel Platform Edition)11

TABLE

1{1Single Processor Systems(continued)

Compaq

ProLiant 1000 Model 3121 (486DX2{66)

Compaq ProLiant 1500 (P-75)

Compaq ProLiant 1500 (1 CPU, P-100)

Compaq ProLiant 1500 (P-133)

Compaq ProLiant 1500 (P-166)

Compaq ProLiant 2000 (1 CPU, P-90)

Compaq ProLiant 2500 (PP-200)

Compaq ProLiant 4000 (1 CPU, P-90)

Compaq ProLiant 4500 (P-100)

Compaq ProLiant 6000 (PP-200)

Compaq ProLiant 7000 (PP-200)

Compaq ProLinea 4/33

Compaq ProLinea 5/133

Compaq ProLinea 575 (P-75)

Compaq ProLinea 6150E

Compaq ProSignia 200 (P-180)

Compaq ProSignia 300 (P-90)

Compaq ProSignia 300 (P-120)

Compaq ProSignia 300 5/150 (P-150)

Compaq ProSignia 300 Model 2100 (P-150)

Compaq ProSignia 500 (P-90)

CompuAdd C4100D Low Pro�le (486DX4-100)

CompuAdd 450

CompuAdd C450D

CompuAdd C450D Low Pro�le

CompuAdd C4100D Low Pro�le (486DX4-100)

CompuAdd C466d

CompuAdd C466D Low Pro�le (486DX2-66)

CompuAdd CP90p

CompuAdd CP90p-LX Low Pro�le

CompuTrend PREMIO Model 5107-AL1 (P-66)

CompuTrend PREMIO Model 5107-AL3 (P-90)12

Hardware

Compatibility List for Solaris 2.6 (Intel Platform Edition)¤ January 1998

TABLE

1{1Single Processor Systems(continued)

Cube

Corp. ATX 466D2

Cube Corp. PowerStation P66

DEC Celebris 590 Low Pro�le (P-90)

DEC Celebris GL5120/ST (P-120)

DEC Celebris XL 5100

DEC Celebris XL 6150 (PP-150)

DEC DECpc 466d2 MTE

DEC DECpc LVp+ (433sx/466d2/4100d4)

DEC Prioris HX 590 (P-90)6

DEC Prioris MX 6200 (PP-200) 7 DEC Prioris MX 6200 (PP-200, 512K) 7 DEC Prioris MX 6200 (PP-200+RAID) 7 DEC Prioris MX 6200 (PP-200+RAID, 512K) 7 DEC V enturis 5133 (P-133)

Dell 433/DE

Dell 450/DE

Dell 466/ME

Dell 466/MX

Dell 466/T

Dell Dimension XPS P90

Dell Dimension XPS P100c

Dell Dimension XPS P120c

Dell Dimension XPS 6150 (PP-150)

Dell Dimension XPS Pro200n (PP-200)

Dell OmniPlex 466

Dell OmniPlex 560

Dell OmniPlex 566

Dell OmniPlex 590

Dell OptiPlex 486/LE MTEHardware Compatibility List for Solaris 2.6 (Intel Platform Edition)13

TABLE

1{1Single Processor Systems(continued)

Dell

OptiPlex 560/L Low Pro�le (P-60)

Dell OptiPlex DGX 590

Dell OptiPlex DGX 5100

Dell OptiPlex DGX 5120

Dell OptiPlex DGX 5133 (P-133)

Dell OptiPlex DGX 5166 (P-166)

Dell OptiPlex GL 575 (P-75)

Dell OptiPlex GL 590 (P-90)

Dell OptiPlex GL 5100 (P-100)

Dell OptiPlex GL 5120 (P-120)

Dell OptiPlex GL 5133 (P-133)

Dell OptiPlex GL 5150 (P-150)

Dell OptiPlex GL+ 575 (P-75)

Dell OptiPlex GL+ 590 (P-90)

Dell OptiPlex GL+ 5100 (P-100)

Dell OptiPlex GL+ 5120 (P-120)

Dell OptiPlex GL+ 5133 (P-133)

Dell OptiPlex GL+ 5150 (P-150)

Dell OptiPlex GM 5133 (P-133)

Dell OptiPlex GM 5150 (P-150)

Dell OptiPlex GM+ 575 (P-75)

Dell OptiPlex GM+ 590 (P-90)

Dell OptiPlex GM+ 5100 (P-100)

Dell OptiPlex GM+ 5120 (P-120)

Dell OptiPlex GM+ 5133 (P-133)

Dell OptiPlex GM+ 5150 (P-150)

Dell OptiPlex GMT 575 (P-75)

Dell OptiPlex GMT 590 (P-90)

Dell OptiPlex GMT 5100 (P-100)14

Hardware

Compatibility List for Solaris 2.6 (Intel Platform Edition)¤ January 1998

TABLE

1{1Single Processor Systems(continued)

Dell

OptiPlex GMT 5120 (P-120)

Dell OptiPlex GMT 5133 (P-133)

Dell OptiPlex GMT 5150 (P-150)

Dell OptiPlex GMT+ 575 (P-75)

Dell OptiPlex GMT+ 590 (P-90)

Dell OptiPlex GMT+ 5133 (P-133)

Dell OptiPlex GMT+ 5150 (P-150)

Dell Optiplex GS 5120 L+M Chassis (P-120)

Dell OptiPlex GS 5133 L+M Chassis (P-133)

Dell Optiplex GS 5150 L+M Chassis (P-150)

Dell OptiPlex GS 5166 MMX L+M Chassis (P-166)

Dell OptiPlex GS 5200 MMX L+M Chassis (P-200)

Dell OptiPlex GS+ 5166

Dell OptiPlex GS+ 5200 (P-200)

Dell OptiPlex GX 575 (P-75)

Dell OptiPlex GX 590 (P-90)

Dell OptiPlex GX 5100 (P-100)

Dell OptiPlex GX 5120 (P-120)

Dell OptiPlex GX 5133 (P-133)

Dell OptiPlex GX 5150 (P-150)

Dell OptiPlex GX Pro 200

Dell OptiPlex GXi 5166 (P-166)

Dell OptiPlex GXi 5200 (P-200)

Dell OptiPlex GXi 5133 L+M Chassis (P-133)

Dell OptiPlex GXi 5133 MMX L+M Chassis (P-133)

Dell OptiPlex GXi 5166 MMX L+M Chassis (P-166)

Dell OptiPlex GXi 5200 MMX L+M Chassis (P-200)

Dell OptiPlex GXi 5233 MT (P-233 MMX)Hardware

Compatibility List for Solaris 2.6 (Intel Platform Edition)15

TABLE

1{1Single Processor Systems(continued)

Dell

OptiPlex GXL 575 (P-75)

Dell OptiPlex GXL 590 (P-90)

Dell OptiPlex GXL 5100 (P-100)

Dell OptiPlex GXL 5120 (P-120)

Dell OptiPlex GXL 5133 (P-133)

Dell OptiPlex GXL 5150 (P-150)

Dell OptiPlex GXL 5166 (P-166)

Dell OptiPlex GXM 575 (P-75)

Dell OptiPlex GXM 590 (P-90)

Dell OptiPlex GXM 5100 (P-100)

Dell OptiPlex GXM 5120 (P-120)

Dell OptiPlex GXM 5133 (P-133)

Dell OptiPlex GXM 5150 (P-150)

Dell OptiPlex GXM 5166 (P-166)

Dell OptiPlex GXMT 575 (P-75)

Dell OptiPlex GXMT 590 (P-90)

Dell OptiPlex GXMT 5100 (P-100)

Dell OptiPlex GXMT 5120 (P-120)

Dell OptiPlex GXMT 5133 (P-133)

Dell OptiPlex GXMT 5150 (P-150)

Dell OptiPlex GXMT 5166 (P-166)

Dell OptiPlex XL 575 (P-75)

Dell OptiPlex XL 590 (P-90)

Dell OptiPlex XL 5100 (P-100)

Dell OptiPlex XL 5120 (P-120)

Dell OptiPlex XM 575 (P-75)

Dell OptiPlex XM 590 (P-90)

Dell OptiPlex XM 5100 (P-100)

Dell OptiPlex XM 5120 (P-120)

Dell OptiPlex XMT 575 (P-75)16

Hardware

Compatibility List for Solaris 2.6 (Intel Platform Edition)¤ January 1998

TABLE

1{1Single Processor Systems(continued)

Dell

OptiPlex XMT 590 (P-90)

Dell OptiPlex XMT 5100 (P-100)

Dell OptiPlex XMT 5120 (P-120)

Dell OptiPlex XMT 5133 (P-133)

Dell PowerEdge 466/XE

Dell PowerEdge SP 590

Dell PowerEdge 2100 (PP-180)

Dell PowerEdge 2100 (PP-200)

Dell SP5100-2 (P-100)

Diversi�ed Technologies (DTI) LBE4520 (P-90)

Diversi�ed Technologies (DTI) LBE4520 (P-100)

DTK FEAT-39 (DX4-100)

DTK QUIN-35D PCI (P-90)

DTK QUIN-35M PCI (P-90)

DTK QUIN-54/I (P-133)

EIS Computers \The Client" (486/66 VLB)

EIS Computers \The Client P60" (P-60)

EIS Computers \The Developer " (486/66 EISA/VLB)

EIS Computers \The Developer P90" (P-90 PCI)

EIS Computers \The Developer P90i" (P-90 PCI)

EIS Computers \The Developer P100" (P-100 PCI)

EIS Computers \The Developer P100i" (P-100 PCI)

EIS Computers \The Developer P120" (P-120 PCI)

EIS Computers \The Developer P120i" (P-120)

EIS Computers \The Developer P120s" (P-120)

EIS Computers \The Developer P133" (P-133)

EIS Computers \The Developer P133i" (P-133)

EIS Computers \The Developer P133s" (P-133)

EIS Computers \The Developer-Pro 150i" (PP-150)

EIS Computers \The Developer-Pro 150s" (PP-150)

EIS Computers \The Developer-Pro 200s"Hardware

Compatibility List for Solaris 2.6 (Intel Platform Edition)17

TABLE

1{1Single Processor Systems(continued)

Elonex

MT5166-I (P-166)

Elonex PC-590-I

Elonex PT 62233AX AMD (K6-233)

Elonex PT 62266 II (PII{266)

Everex Step DP (tested w/ 1 CPU, P-90)

Everex Step DPi (P-133)

Fujitsu FM-5000SV Model 250 (P-166)

Fujitsu FMV-466D (486DX2-66)

Fujitsu FMV-575D4L (P-75)

Fujitsu FMV-575D5 (P-75)2

Fujitsu FMV-590D3 (P-90)

Fujitsu FMV-590DE (P-90)

Fujitsu FMV-5100D4L (P-100)

Fujitsu FMV-5100D6 (P-100)

Fujitsu FMV-5100DE3 (P-100) 2 Fujitsu FMV-5133D5 (P-133) 2 Fujitsu FMV-5133D6 (P-133)

Fujitsu FMV-5133D7 (P-133)

Fujitsu FMV-5133DE3 (P-133) 2 Fujitsu FMV-5133DE4 (P-133)

Fujitsu FMV-5133T3 (P-133) 2 Fujitsu FMV-5150T4 (P-150)

Fujitsu FMV-5166D5 (P-166)

Fujitsu FMV-5166D6 (P-166)

Fujitsu FMV-5166D8M (P-166 MMX)

Fujitsu FMV-5166DE4 (P-166)

Fujitsu FMV-5166DE5 (P-166)

Fujitsu FMV-5166T5 (P-166)

Fujitsu FMV-5200DE6 (P-200)18

Hardware

Compatibility List for Solaris 2.6 (Intel Platform Edition)¤ January 1998

TABLE

1{1Single Processor Systems(continued)

Fujitsu

FMV-5200T4 (P-200)

Fujitsu FMV-6150T3 (PP-150)

Fujitsu FMV-6200T4 (PP-200)

Fujitsu FMV-6200T5 (PP-200)

Fujitsu FMV-6233D8 (PII-233)

Fujitsu FMV-6266T6 (PII-266)

Fujitsu GranPower5000 Model 560S (PP-200)

Fujitsu ICL ErgoPro Desktop X450-90 (P-90)

FutureTech 4100V (486 DX4-100)

FutureTech 462iV (i486 DX2-66)

FutureTech 5601P (P-60)

FutureTech FTS4414 (AMD486 DX-40)

Gateway 2000 486/33E

Gateway 2000 4DX2-66 (low pro�le)3

Gateway 2000 4DX2-66E

Gateway 2000 4DX2-66V

Gateway 2000 4SX-33 (low pro�le) 3 Gateway 2000 G6-150 (PP-150)

Gateway 2000 G6-200 (PP-200)

Gateway 2000 P4D-66 3 Gateway 2000 P4D-100 (486DX4-100)

Gateway 2000 P5-60

Gateway 2000 P5-66 3 Gateway 2000 P5-75 (P-75)Hardware Compatibility List for Solaris 2.6 (Intel Platform Edition)19

TABLE

1{1Single Processor Systems(continued)

Gateway

2000 P5-90 Tower

Gateway 2000 P5-120 Tower

Gateway 2000 P5-100 (P-100)8

Gateway 2000 P5-100 new revised motherboard (P-100)

Gateway 2000 P5-100XL (P-100) 8 Gateway 2000 P5-120 (P-120) 9

Gateway 2000 P5-133XL (P-133)

GCH Systems EasyData 590 (P4C-90)

GCH Systems Aegis 466 (i486DX2-66)

GCH Systems Aegis 466ES (i486DX2-66)

GoldStar GT51P PCI (P-60)

Hitachi FLORA 1010DK (P-60)

Hitachi FLORA 1010DL

Hitachi FLORA 1010DM (P-100)

Hitachi FLORA 1010DN

Hitachi FLORA DS1 (P-75)

Hitachi FLORA DS1 (P-100)

Hitachi FLORA DS1 (P-133)

Hitachi FLORA SA1 (P-166)

Hitachi FLORA SA1 (P-200)

Hitachi FLORA SM1 (PP-200)

HP NetServer 4d/66LE (486DX2-66) 10 HP NetServer 4d/66LM 11

HP NetServer 5/66 LC (P-66)

HP NetServer 5/66 LF (P-66)

HP NetServer 5/133 LS (P-133)

HP NetServer LC 5/66 (P-66)20

Hardware

Compatibility List for Solaris 2.6 (Intel Platform Edition)¤ January 1998

TABLE

1{1Single Processor Systems(continued)

HP NetServer LM 5/100 (P-100)

HP V ectra VL 5/90 Series 3 PC (P-90)

HP V ectra VL2 4/100 PC (486DX4-100)

HP V ectra VL2 5/60 PC (P-60)

HP V ectra VL2 5/90 PC (P-90)

HP V ectra VT 6/150 PC (PP-150)

HP V ectra XA 6/200 PC (PP-200)

HP V ectra XM 5/90 Series 3 (P-90)

HP V ectra XM 5/100 Series 4 PC (P-100)

HP V ectra XM2 4/66i PC (486DX2-66)

HP V ectra XU 5/90 PC (P-90)

HP V ectra XU 5/90C PC (P-90)12

HP V ectra XU 5/133C PC (P-133)

HP V ectra XU 6/150 PC (PP-150)

HP V ectra XU 6/200 PC (PP-200)

Hyundai Phantom P-90 Desktop

I BUS ORCA (486DX4/100)

I BUS SHARK (P-133)

IBM Aptiva H5F (P-150)

IBM PC Server 310 Model 8639-ODO (P-133)

IBM PC Server 310 Model 8639-OE4 (P{200 )

IBM PC Server 310 Model 8639-OEO (P-166)

IBM PC Server 310 Model 8639-OEV P-166)

IBM PC Server 310 Model 8639-OXT P-75)

IBM PC Server 315 Model 8638-PJV (PP-180)

IBM PC Server 315 Model 8638-PSV (PP-200)

IBM PC Server 320 Model 8640-EEV (P-166)Hardware

Compatibility List for Solaris 2.6 (Intel Platform Edition)21

TABLE

1{1Single Processor Systems(continued)

IBM PC Server 320 Model 8640-ODO (P-133)

IBM PC Server 320 Model 8640-ODV (P-133)

IBM PC Server 320 Model 8640-ONJ (486DX2-66)

IBM PC Server 320 Model 8640-OPT (P-180)

IBM PC Server 325 Model 8640-ES0 (PP-200)

IBM PC Server 325 Model 8639-EJO (PP-180)

IBM PC Server 325 Model 8640-ESV (PP-200)

IBM PC Server 330 Model 8640-EM2 (PP-200)

IBM PC Server 330 Model 8640-ESS (PP-200)

IBM PC Server 330 Model 8640-PMO (PP-200)

IBM PC Server 500 Model 8641-OYR (P-90)

IBM PC Server 500 Model 8641-OYT (P-90)

IBM Personal Computer 300 Series Model 6571

IBM Personal Computer 300 Series Model 6575

IBM Personal Computer 300 Series Model 6581

IBM Personal Computer 300 Series Model 6585

IBM Personal Computer 300 GL Model 6282-34U (P{166)

IBM Personal Computer 300 XL Model 6588{10U (PII{233)

IBM Personal Computer 330 Model 6576 (P-75)

IBM Personal Computer 330 Model 6576 (P-133)

IBM Personal Computer 340 Model 6560-79M (P-133)

IBM Personal Computer 350 Model 6587-LBV (P-200 MMX)

IBM Personal Computer 350-100DX4

IBM Personal Computer 360 Model 6589 (PP-200)

IBM Personal Computer 360 Model 6589-12U (PP-200)

IBM Personal Computer 360 Model 6598 (PP-150)

IBM Personal Computer 365 Model 6589-10U (PP-200)22

Hardware

Compatibility List for Solaris 2.6 (Intel Platform Edition)¤ January 1998

TABLE

1{1Single Processor Systems(continued)

IBM Personal Computer 365 Model 6589-12U (PP-200)

IBM Personal Computer 700 Series Model 6875

IBM Personal Computer 730 Model 6877-KAZ (P-100)

IBM Personal Computer 750 Model 6885 (P-75)

IBM Personal Computer 750 Model 6885-35H (P-75)

IBM Personal Computer 750 Model 6885-JOM (P-90)

IBM PS/2 Model 76 (9576-xxx)

IBM PS/2 Model 95 XP486 (9595-OL)

IBM PS/2 Model 95 XP486 (9595-OM)

IBM PS/2 Server 95 (9595-3QT)6

IBM PS/2 Server 95 (9595-OPT) 6 IBM PS/ValuePoint 466DX2/D

IBM PS/ValuePoint P60/D

IBM PS/ValuePoint Performance Series 486 DX2/66 Dp

Industrial CPU Systems PC (P-133)

Infotel Ultra P5-75 PCI

Infotel Ultra P5-90 PCI Minitower

Infotel Ultra P5-100 PCI

Infotel Ultra P5-120 PCI

Intel Advanced/AL (Aladdin-Triton) (P-90)

Intel Advanced/AS (Atlantis) (P-166)

Intel Advanced/ATX

Intel Advanced/EV Pentium/100

Intel Advanced/EV (Endeavor) (P-75)

Intel Advanced/EV (Endeavor) (P-90)HardwareCompatibility List for Solaris 2.6 (Intel Platform Edition)23

TABLE

1{1Single Processor Systems(continued)

Intel

Advanced/EV (Endeavor) (P-100)

Intel Advanced/EV (Endeavor) (P-120)

Intel Advanced/EV (Endeavor) (P-133)

Intel Advanced/EV (Endeavor) (P-150)

Intel Advanced/EV (Endeavor) (P-166)

Intel Advanced/ML (Marl) (P-133)

Intel Advanced/MN (Morrison) (P-100)

Intel Advanced/PO (P-133)

Intel Advanced/RH (Rhinestone) (P-133)

Intel Advanced/RH (Rhinestone) (P-200)

Intel Advanced/RH (Rhinestone) (P-200 MMX)

Intel Advanced/VS (V enus) (PP-180)

Intel Advanced/VS (V enus) (PP-200)

Intel Advanced/ZE Mini-tower (P-100)

Intel Advanced/ZP (Zappa-Triton) (P-90)

Intel ALTserver Altair (P-150)

Intel ALTserver Altair (P-166)

Intel AP450GX MP Server (1 CPU version) (PP-200)

Intel Express 486/DX33

Intel Express Pentium/60

Intel Express Pentium/90

Intel L486-Series Professional GX (486DX2-66)

Intel Pentium Pro Performance/AU

Intel Pentium Pro Performance/AU ATX

Intel Performance/AU (PP-180)

Intel Performance/AU (PP-200)

Intel Premiere/PCI LX (Plato) (P-90)

Intel R440FX UP Server (PP-200)

Intel RC440FX UP Server (PP-200)24

Hardware

Compatibility List for Solaris 2.6 (Intel Platform Edition)¤ January 1998

TABLE

1{1Single Processor Systems(continued)

Intergraph

TD-1 (486DX2-66)

Intergraph TD-2 (P-66)

Intergraph TD-3 (P-90)

Intergraph TD-3 (P-100)

Intergraph TD-30 (P-90)13

Intergraph TD-300 (PP-150)

Intergraph TD-300 (PP-200)

Intergraph TD-310 (PP-200)

Intergraph TD{320 (PP-200)

Intergraph TD-325 (Pentium II-266)

Inves BS-486-VS i486 DX2-50

IPEX Desktop Model PCI-I-133 (P-133)

Leading Edge Fortiva Series 3000 (486DX2-50)

Leading Edge Fortiva Series 4000 (Cyrix 486DLC-40) 1 Leading Edge Fortiva Series 5000 (486DX2-66)

Leading Edge MT 6000 (P-90)

Leading Edge MT 6000 Tower (P-90)

Leading Edge Valience Desktop DT4000

Metrologie P60 Tower (Intel Express P-60)

Metrologie Premiere/PCI P60 Desktop (Intel Mercury)

Microbus European Data Systems iBOX (486DX-33) 14 Micron 486PCI MAGNUM (486 DX4-100)

Micron ClientPro MTA 200 (P-200)

Micron ClientPro MTE 200 (P-200 MMX)

Micron ClientPro MTE 200 (P-200 MMX) (BusLogic SCSI)

Micron ClientPro XLU (Pentium II-233)

Micron Home MPC (P-90)

Micron Home MPC (P-166)Hardware Compatibility List for Solaris 2.6 (Intel Platform Edition)25

TABLE

1{1Single Processor Systems(continued)

Micron

Magnum Plus Pro200 IDE version (PP-200)

Micron Magnum Plus Pro200 SCSI version (PP-200)

Micron Magnum Plus Pro200 2940U SCSI version (PP-200)

Micron Millennia 100 (P-100)

Micron Millennia P166 (P-166)

Micron Millennia LXE (P-200 MMX)

Micron Millennia MME (P-200 MMX IDE)

Micron Millennia Plus (P-133)

Micron Millennia Pro Plus (P-200)

Micron Millennia XRU (PII-266)

Micron P90PCI PowerStation15

Micron P90PCI PowerStation Mini-Tower, Plug and Play (P-90)

Micron PowerServer SMP (P-90)

Micron PowerServer SMP (P-133)

Midwest Micro (P-75 PCI)

Midwest Micro (P-100 PCI)

Midwest Micro (P-120 PCI)

Midwest Micro Desktop 486DX2-66 (486DX2/66)

Midwest Micro Minitower P5-90

Mitsubishi Electric FT2200 (PP-200)

Mitsubishi Electric FT2400 (PP-200+RAID)

NCR 3333 (486DX2/66)

NCR 3269-200 (PP-200)

NCR 3269-300 (PP-200)

NCR S16 (PP-200)

NCR WorldMark 4300 1CPU (1 CPU, PP-200 512K)

NEC Express 5800 (P-120)

NEC Express 5800/120Pro (PP-200)

NEC Powermate Pro-2200 (PP-200)

NEC Powermate VE (P-133)

NJA Triton T-01W (P-133)26

Hardware

Compatibility List for Solaris 2.6 (Intel Platform Edition)¤ January 1998

TABLE

1{1Single Processor Systems(continued)

Olivetti

M4-82 16

Olivetti M6-420

Olivetti M6-440 17 Olivetti M6-450 17 Olivetti M6-460 17 Olivetti M6-640 6 Olivetti M6-750

16 18

Olivetti M6-760

16 18

Olivetti M6-770

16 18

Olivetti M6-850 1 6 Olivetti M6-860 6 Olivetti M6-880 6 Olivetti NETSTRADA 1000 Pro 200 M1 (PP-200)

Olivetti NETSTRADA 1000 Pro 200 M1 (PP-200+RAID)

Olivetti NETSTRADA 3000 Pro 200 M1 (PP-200)

Olivetti NETSTRADA 3000 Pro 200 M32+ (PP-200+RAID)

Olivetti NETSTRADA 5000 Pro 200 (PP-200+RAID)

Olivetti NETSTRADA 7000 Pro 200

Olivetti SNX-140 16 Olivetti SNX-160UP (P-90)

OMEGABYTE SolarSTATION XP 75 (P-75)

OMEGABYTE SolarSTATION XP 90 (P-90)

OMEGABYTE SolarSTATION XP 100 (P-100)

OMEGABYTE SolarSTATION XP 120 (P-120)

OMEGABYTE SolarSTATION XP 133 (P-133)

OMEGABYTE SolarSTATION XP 166 (P-166)

OMEGABYTE SolarSTATION XPR 150 (PP-150)

OMEGABYTE SolarSTATION XPR 200 (PP-200)Hardware

Compatibility List for Solaris 2.6 (Intel Platform Edition)27

TABLE

1{1Single Processor Systems(continued)

Paci�c

Micro Data Mast Workgroup 800 RAID Subsystem (P-100, 512K)

Packard Bell Axcel Series19

Packard Bell Executive Series 19 Packard Bell Force Series 19 Packard Bell Legend Series 19 Packard Bell Pack-Mate Series 19 Packard Bell PRO Series 19 Packard Bell NEC MultiMedia F170 (P-166)

Packard Bell NEC Z-Station GT Pro (PP-200)

Peacock-AG AT 486 DX-40 Professional Plus Desktop

Peacock-AG LAN-Station AT 486 DX-40 LN4

Research Machines PC-425S (486SX/25)

Research Machines PC-450S Accelerator (486SX2-50)

Research Machines PC-560 Accelerator (P-60)

Research Machines PC-590 Professional (P-90) 20 R Style Proxima (P-90)

Samsung Magic Power SPC8500(P-90)

Samsung Magic Power SPC8500 (P-133)

Samsung Magic Power SPC8500PA (P-133)

Samsung SWS 520/90 (P-90)

Samsung SWS 520/100 (P-100)

Samsung SWS 520/133 (P-133)

Siemens ANL Siix Server 1 (486 DX2-50)28

Hardware

Compatibility List for Solaris 2.6 (Intel Platform Edition)¤ January 1998

TABLE

1{1Single Processor Systems(continued)

Siemens

Nixdorf AG PCD-5H (P-133 Desktop)

Siemens Nixdorf AG PRIMERGY 150 (P-120)

Siemens Nixdorf AG PRIMERGY 151 (P-166)

Siemens Nixdorf AG PRIMERGY 060 (PII-266)

Siemens Nixdorf AG PRIMERGY 160 (PP-200)

Siemens Nixdorf AG PRIMERGY 160 V ersion K423 V7xx (PP-200)

Siemens Nixdorf AG Scenic Pro C5 (P-166)

Siemens Nixdorf AG Scenic Pro C6 (PP-200)

Siemens Nixdorf AG Scenic Pro M5 (PP-200)

Siemens Nixdorf AG Scenic Pro M6 (PP-200)

Siemens Nixdorf AG Scenic Pro M6 (PP-200)

Siemens Nixdorf PCD-4H/VL (486DX2-50)

Siemens Nixdorf PCD-4H/VL (486DX2-66)

Siemens Nixdorf PCD-4H/PCI (486DX2-66)

Siemens Nixdorf PCD-5H (P-60 PCI)21

Siemens Nixdorf PCD-5H (P-90)

Siemens Nixdorf PCD-5T

Siemens Nixdorf PCE-5S

TAGRAM Platinum (P-66)

TAGRAM ThunderBolt (P-66)

TAKAOKA Electric MiNT PC5133s3

TAKAOKA Electric MiNT PC590d2 Desktop (P-90)

TAKAOKA Electric MiNT PC590t2 Tower (P-90)

TAKAOKA Electric MiNT PC5166d4 Desktop (P-166)

TAKAOKA Electric MiNT PC5166t4 Tower (P-166)

TAKAOKA Electric MiNT PC5200d4 Desktop (P-200)

TAKAOKA Electric MiNT PC5200t4 Tower (P-200)

TAKAOKA Electric MiNT PC6200d Desktop (PP-200)Hardware

Compatibility List for Solaris 2.6 (Intel Platform Edition)29

TABLE

1{1Single Processor Systems(continued)

Toshiba

Desktop BREZZA 5200MB PV1010JA (P-200)

Toshiba Desktop Equium 5200D (P-200 MMX)

Toshiba J-3100 PV (486SX-25 ODP)

Toshiba J-3100 PV2 (486DX2-66)

Tulip 4-Series DE PCI (486DX2-66)

Tulip 5-Series DE PCI (P-90)

Tulip 4-Series DE EISA (486DX2-66)

Tulip 4-Series DS PCI (486DX2-66)

Tulip 5-Series DS PCI (P-90)

Tulip 4-Series DS EISA (486DX2-66)

Tulip 4-Series DT ISA (486DX2-66)

Tulip 4-Series DT PCI (486DX2-66)

Tulip 5-Series DT PCI (P-90)

Tulip 4-Series TR EISA (486DX2-66)

Tulip Vision Line DE5-200 (PP-200)22

Tulip Vision Line DS6-200 (PP-200) 23 Tulip Vision Line DS6-200S (PP-200) 24 Tulip Vision Line DT5-133 (P-133) 25 Tulip Vision Line DT5-133S (P-133) 26 Tulip Vision Line TR6-SMP1 (PP-200) 27 Unisys Aquanta DM II-CMT 57574 (P-75)

Unisys Aquanta DM II-CMT 515074 (P-150)

Unisys Aquanta DM II-CMT 520074 (P-200)

Unisys Aquanta DM/6 II-CMT 618072 (PP-180)

Unisys Aquanta DM/6 II-CMT 620072 (PP-200)

Unisys Model SVD-II P166 w/ 2940SCSI

Unisys Model SVD-II P166 w/ int 7870SCSI

Unisys U6000/100

Unisys U6000/300

Unisys U6000/DT2 30

Hardware

Compatibility List for Solaris 2.6 (Intel Platform Edition)¤ January 1998

TABLE

1{1Single Processor Systems(continued)

Viglen

Contender Professional 4DX266

Viglen Genie 2 (PII-266 MMX)

Viglen Genie PCI Pro 200

Viglen Genie PCI Professional 4DX266

Viglen Genie PCI (P-133)

Viglen Genie PCI Tower (P-90)

Viglen LX Server (P-200)

Viglen LX Server Pro (PP-200)

Viglen XX Pro Server (PP-200)

WellStone EZ-Go Type-1 Tower (P-90)

WellStone EZ-Go Type-2 Tower (P-120)

WellStone SWS 5090 (P-90)

WellStone SWS 6200 Tower (PP-200)

Wyse Decision 486se

Wyse Decision 486Gsi (DX2/66)

Wyse Series 6000i Model 650

Wyse Series 6000i Model 665

Zenith Data Systems Z-Select 100 XE Minitower (486DX2-66)

Zenith Data Systems Z-Select PT (P-60)

Zenith Data Systems Z-Server EL Pro (PP-200)

Zenith Data Systems Z-Server EX P90E Model 1000

Zenith Data Systems Z-Server EX P90E Model 1000A

Zenith Data Systems Z-Server LT 433DE Model 1000

Zenith Data Systems Z-Server LT 433DE Model 1000A

Zenith Data Systems Z-Server LT 450DE Model 1000

Zenith Data Systems Z-Server LT 450DE Model 1000A

Zenith Data Systems Z-Server LT 466XE Model 1000

Zenith Data Systems Z-Server LT P60E Model 1000

Zenith Data Systems Z-Server LT P60E Model 1000AHardware

Compatibility List for Solaris 2.6 (Intel Platform Edition)31

TABLE

1{1Single Processor Systems(continued)

Zenith

Data Systems Z-Server MX (P-100)

Zenith Data Systems Z-Server MX+Mylex (P-100)

Zenith Data Systems Z-Server WG P90 (P-90)

Zenith Data Systems Z-Station 510 Minitower (486DX4-100)

Zenith Data Systems Z-Station EL (P-133)

Zenith Data Systems Z-Station EX Model II (P-90)

Zenith Data Systems Z-Station GT-575 (P-75)

Zenith Data Systems Z-Station GT-5100

Zenith Data Systems Z-Station GT-5120

Zenith Data Systems Z-Station GT-5133 (P-133)

Zenith Data Systems Z-Station GT-5150

Zenith Data Systems Z-Station GT-5166

Zenith Data Systems Z-Station GT Pro (PP-200 IDE)

Zenith Data Systems Z-Station GT Pro-S (PP-200 SCSI)

Zenith Data Systems Z-Station LX Pro (PP-180 )

Zenith Data Systems Z-Station LX Pro-S (PP-180 SCSI)

Zenith Data Systems Z-Station LX Pro (PP-200)

Zenith Data Systems Z-Station LX Pro-S (PP-200 SCSI)

Zenith Data Systems Z-Station VP (486DX4/100)

Zenith Data Systems Z-Station VP (P-90)

Zenith Data Systems Z-Station VP (P-100)

Zenith Data Systems Z-Station VP (P-120)

Zenith Data Systems Z-Station VP (P-133) 1.

Requires substituting the video card with one supported by Solaris Intel Platform Edition.

2. Requires substituting the network card with one supported by Solaris Intel Platform Edition.

3. Must use a CD-ROM drive supported by Solaris Intel Platform Edition.

4. This model is an MP server but has only been tested with one CPU.

5. Additional con�guration is required to install the Solaris 2.6 software on this system; refer to the

notes on \Memory Mapping Problems" in Solaris 2.6 (Intel Platform Edition) Release Notes for

information.

6. Server System. Integrated video currently only works in 640x480 VGA mode.

7. Refer to the certi�cation report for this system athttp://access1.sun.com/certify/reports/DEC/.

8. Requires non-default BIOS settings for proper operation.

9. The three-disk CD-ROM changer is not supported at this time.

10. Select \Trident 9000" when con�guring the display adapter, and be sure to upgrade the video RAM

on the motherboard.

11. System must be upgraded to a minimum of 1-Mbyte video memory and a minimum of 32-Mbytes

system memory.32

Hardware

Compatibility List for Solaris 2.6 (Intel Platform Edition)¤ January 1998

TABLE

1{1Single Processor Systems(continued)

12. Some versions may require a future Driver Update to support integrated video due to a

manufacturer’s part change.

13. PC Card support is planned for a future Driver Update.

14. The design of the Cache controller requires that you map out the memory range used by the SCSI

controller, or the system will not work; the on-board hardware watchdog circuit R39 must also be

disabled.

15. Warning: FLASH BIOS must be write-protected before attempting to install the Solaris software;

remove jumper JP9 on the motherboard and use BIOS revision -10 or later.

16. Only tested with vendor’s ATI Mach32 video option.

17. Integrated audio chip is not currently supported.

18. Must set the Adaptec SCSI BIOS to address CC000.

19. This series of machines comes in various models and con�gurations. If the FCC ID label on the back

panel of your machine contains one of the three-digit codes 430, 450, 470, 520, or 550, then it is

based on a platform that was tested for compatibility and should run Solaris 2.6 Intel Platform

Edition. However, ensure that other optional equipment and subsystems on your speci�c model are

listed in this document.

20. The newer version of this system had BIOS compatibility issues at the time of test. Also, attach the

CD-ROM to the primary IDE channel.

21. Built-in ATI video card currently only supported in 43-Hz mode.

22. For Solaris compatibility, specify an STB S3 Trio video system by requesting option

DE-15-200-2-SFC12-E16/1-DU-3P4I-U at time of order.

23. For Solaris compatibility, specify an STB S3 Trio video system by requesting option

DS-16-200-1.2-IFC8-E32/1S-DF-4P4I-U at time of order.

24. For Solaris compatibility, specify an STB S3 Trio video system by requesting option

DS-16-200-2-SFC8-E32/1S-DF-4P4I-U at time of order.

25. For Solaris compatibility, specify an STB S3 Trio video system by requesting option

DT-15-133-1.2-IFC8-E16/1S-CU-2P2I-U at time of order.

26. For Solaris compatibility, specify an STB S3 Trio video system by requesting option

DT-15-133-2-SFC8-E16/1S-CU-2P2I-U at time of order.

27. For Solaris compatibility, specify an STB S3 Trio video system by requesting option

TR-16-200-4.0W-SFC4-P64/1S-4P2I-U at time of order. Note

-The number of CPUs following each entry indicates the number of

processors in the multiprocessor system as tested. Hardware

Compatibility List for Solaris 2.6 (Intel Platform Edition)33

TABLE

1{2Multiprocessor Systems (SMP) Acer

AcerAltos 7000/P (2 CPUs, P-90)

AcerAltos 9000 Pro (2 CPUs, PP-200)

AcerAltos 19000 SMP (2 CPUs, PP-200)

AcerAltos 19000 SMP (2 CPUs, PP-200 w/ RAID)

Acer AcerFrame Model 3000MP (2 CPUs)

ALR Evolution (2 CPUs, PP-200)

ALR Evolution Dual6 (2 CPUs, PP-200)

ALR Evolution V STe/75 (2 CPUs, P-75)

ALR Evolution Q/MP2 100 (2 CPUs, P-100)

ALR Proveisa SMP (2 CPUs)

ALR Rack Mountable Revolution Quad6-200 w/ 256 cache (4 CPUs, PP-200)

ALR Revolution 2X (2 CPUs, PII-266)

ALR Revolution 6x6 (3 CPUs, PP-200)

ALR Revolution 6x6 (6 CPUs, PP-200)

ALR Revolution Dual6 (2 CPUs, PP-200)

ALR Revolution MP 100 (2 CPUs, P-100)

ALR Revolution MP 166 (2 CPUs, P-166)

ALR Revolution MP II (2 CPUs, P-166)

ALR Revolution MP II (2 CPUs, P-200)

ALR Revolution MP Pentium 90 (2 CPUs)

ALR Revolution Q-SMP PCI-V ersion (2 CPUs, P-100)

ALR Revolution Q-SMP PCI-V ersion (4 CPUs, P-166)

ALR Revolution Q-SMP Pentium/90 (2, 3, & 4 CPUs)

ALR Revolution Q-SMP Pentium/100 (2 CPUs)

ALR Revolution Q-SMP Pentium/100 (4 CPUs)

ALR Revolution Quad6-200 (2 CPUs, PP-200)

ALR Revolution Quad6-200 (3 CPUs, PP-200)

ALR Revolution Quad6-200 (4 CPUs, PP-200)

ALR Revolution VQ/4SMP (4 CPUs, P-166)

Amdahl Envista Server (4 CPUs, PP-166)

American Megatrends Titan-II PCI EISA (2 CPUs)34

Hardware

Compatibility List for Solaris 2.6 (Intel Platform Edition)¤ January 1998

TABLE

1{2Multiprocessor Systems (SMP)(continued)

AMG Pro200SMP-2N Server (2 CPUs, PP-200)

AST Manhattan SMP 486/33 (4 CPUs)

AST Manhattan SMP P/60 (4 CPUs)

AST Manhattan P5090 (2 CPUs, P-90)1

AST Manhattan P5100 (2 CPUs)

AST Manhattan P5133 (2 CPUs)

AST Manhattan S6200 Model 2003LC (2 CPUs, PP-200)

AST Manhattan V5090 (2 CPUs, P-90) 1 2

AST Manhattan V5100 (2 CPUs)

AST Premmia GX (2 CPUs, P-90) Integrated E-IDE

AST Premmia GX (2 CPUs, P-90) Integrated SCSI 2 AST Premmia GX (2 CPUs, P-100)

AST Premmia GX (2 CPUs, P-133)

AT&T GIS Globalyst S40 (4 CPUs, P-100)

Austin Direct Af�nity SE (2 CPUs, P-90)

C&S V ertriebs GmbH (2 CPUs, P-90, EISA/PCI)

C&S V ertriebs GmbH AMICUS Strategy (2 CPUs, P-133)

Compaq Professional Workstation 5000 (2 CPUs, PP-200)

Compaq Professional Workstation 6000 (2 CPUs, PII-266)

Compaq Professional Workstation 8000 (2 CPUs, PP-200)

Compaq Professional Workstation 8000 (4 CPUs, PP-200)

Compaq ProLiant 800 (2 CPUs, PP-200)

Compaq ProLiant 850R (2 CPUs, PP-200)

Compaq ProLiant 1500 (2 CPUs, P-133)

Compaq ProLiant 1500 (2 CPUs, PP-200)

Compaq ProLiant 2000 (2 CPUs, P-90)

Compaq ProLiant 2500 (2 CPUs, PP-200)HardwareCompatibility List for Solaris 2.6 (Intel Platform Edition)35

TABLE

1{2Multiprocessor Systems (SMP)(continued)

Compaq

ProLiant 4000 (4 CPUs, P-90)

Compaq ProLiant Server 4500/166 (2 CPUs, P-166)

Compaq ProLiant Server 4500/166 (4 CPUs, P-166)

Compaq ProLiant 5000 (4 CPUs, PP-166)3

Compaq ProLiant 5000 (4 CPUs, PP-200)

Compaq ProLiant 6000 (2 CPUs, PP-200)

Compaq ProLiant 6000 (4 CPUs, PP-200)

Compaq ProLiant 7000 Dual (2 CPUs, PP-200)

Compaq ProLiant 7000 Quad (4 CPUs, PP-200)

Data General Aviion 3000 Server (2 CPUs, P-100)

DEC Celebris XL 590DP (2 CPUs, P-90)

DEC Celebris XL 5166DP (2 CPUs, P-166)

DEC Prioris HX 590DP (2 CPUs, P-90)

DEC Prioris MX 6200 (2 CPUs, PP-200) 4 DEC Prioris MX 6200 (2 CPUs, PP-200, 512K) 7 DEC Prioris MX 6200 (2 CPUs, PP-200+RAID) 7 DEC Prioris MX 6200 (2 CPUs, PP-200+RAID, 512K) 7 DEC Prioris XL Server 5200DP (2 CPUs, PP-200)

DEC Prioris ZX 6166 MP2 (2 CPUs, PP-166)

DEC Prioris ZX 6200 MP2 (2 CPUs, PP-200)

Dell OptiPlex DGX 590 (2 CPUs, P-90)

Dell OptiPlex DGX 5100 (2 CPUs, P-100)

Dell OptiPlex DGX 5120 (2 CPUs, P-120)

Dell OptiPlex DGX 5133 (2 CPUs, P-133)

Dell OptiPlex DGX 5166 (2 CPUs, P-166)

Dell OptiPlex GX Pro 180 (2 CPUs, PP-180)

Dell OptiPlex GX Pro 200 (2 CPUs, PP-200)

Dell PowerEdge 4100 (2 CPUs, PP-180)

Dell PowerEdge 4100 (2 CPUs, PP-200)

Dell PowerEdge SP 5100 (2 CPUs, P-100)

Dell PowerEdge XE 590-2 with DSA (2 CPUs, P-90)36

Hardware

Compatibility List for Solaris 2.6 (Intel Platform Edition)¤ January 1998

TABLE

1{2Multiprocessor Systems (SMP)(continued)

Diversi�ed

Technologies (DTI) LBE-4520 DP (2 CPUs, P-90)

DTK QUIN-52M DP90 (2 CPUs, P-90)

EIS Computers Mega Developer 200-4 (4 CPUs, PP-200)

EIS Computers Monster Developer Pro (2 CPUs, PP-200)

EIS Computers Monster Developer Pro (4 CPUs, PP-200 512K)

EIS Computers Super Developer Pro (2 CPUs, PP-200)

EIS Computers Super Developer Pro II (2 CPUs, PP-200 512K)

EIS Computers \The Developer " (2 CPUs, P-90 MP)

EIS Computers \The Developer " (2 CPUs, P-100 MP)

EIS Computers \The Developer-Pro 200" (2 CPUs, PP-200)

EIS Computers \The Server " (2 CPUs, P-90 MP)

EIS Computers \The Server " (2 CPUs, P-100 MP)

Elonex MT-5133-I (2 CPUs, P-133)

Elonex MTX 62200 (2 CPUs, PP-200)

Everex Step DP (2 CPUs, P-90)

Everex Step DPi (2 CPUs, P-133)

Fujitsu GranPower5000 Model 570S (2 CPUs, PP-200)

Fujitsu GranPower5000 Model 760 (2 CPUs, PP-200)

Hitachi FLORA 3010DV (2 CPUs, P-90)

Hitachi FLORA 3100BP (2 CPUs, P-90)

Hitachi FLORA 3100LP (8 CPUs, P-100)

Hitachi FLORA 3100LP Quad (4 CPUs, P-133)

Hitachi FLORA 3100SP (2 CPUs, P-90)5

Hitachi FLORA SB1 (2 CPUs, PP-200)

Hitachi FLORA SM1 PC 6SM01 1800HA (2 CPUs, PP-180)

Hitachi FLORA SM1 PC 6SM01 18080A (2 CPUs, PP-180 w/ RAID)

Hitachi FLORA SM2 Dual (2 CPUs, PP-200)

Hitachi FLORA SR1 (2 CPUs, PP-200)

Hitachi FLORA SS1 (2 CPUs, PP-200)HardwareCompatibility List for Solaris 2.6 (Intel Platform Edition)37

TABLE

1{2Multiprocessor Systems (SMP)(continued)

HP NetServer 5/66 LM-2 (2 CPUs)1

HP V ectra XU 5/90C PC (2 CPUs, P-90) 6

HP V ectra XU 5/133C PC with Matrox Video (2 CPUs, P-133)

HP V ectra XU 6/150 PC (2 CPUs, P-150)

IBM PC Server 320 Model 8640-EE0 (2 CPUs, P-166)

IBM PC Server 320 Model 8640-EEV (2 CPUs, P-166)

IBM PC Server 320 Model 8640-0Z0 (2 CPUs, P-100)

IBM PC Server 320 Model 8640-0ZV (2 CPUs, P-100)

IBM PC Server 320 Model 8640-1D0 (2 CPUs, P-133)

IBM PC Server 320 Model 8640-1DS (2 CPUs, P-133)

IBM PC Server 320 Model 8640-1Z0 (2 CPUs, P-100)

IBM PC Server 320 Model 8640-MDO (2 CPUs, P-133)

IBM PC Server 320 Model 8640-MDS (2 CPUs, P-133)

IBM PC Server 320 Model 8640-MDV (2 CPUs, P-133)

IBM PC Server 320 Model 8640-MXO (2 CPUs, P-75)

IBM PC Server 320 Model 8640-MXT (2 CPUs, P-75)

IBM PC Server 320 Model 8640-OXO (2 CPUs, P-75)

IBM PC Server 320 Model 8640-OXT (2 CPUs, P-75)

IBM PC Server 320 Model 8640-OYT (2 CPUs, P-90)

IBM PC Server 325 Model 8639-EJO (2 CPUs, PP-180)

IBM PC Server 325 Model 8639-ES0 (2 CPUs, P-200)

IBM PC Server 325 Model 8639-ES0 (2 CPUs, PP-200)

IBM PC Server 325 Model 8639-ESV (2 CPUs, P-200)

IBM PC Server 325 Model 8639-ESV (2 CPUs, PP-200)

IBM PC Server 325 Model 8639-RS0 (2 CPUs, P-200)

IBM PC Server 325 Model 8639-RS0 (2 CPUs, PP-200)

IBM PC Server 325 Model 8640-ESO (2 CPUs, PP-200)

IBM PC Server 325 Model 8640-ESV (2 CPUs, PP-200)38

Hardware

Compatibility List for Solaris 2.6 (Intel Platform Edition)¤ January 1998

TABLE

1{2Multiprocessor Systems (SMP)(continued)

IBM PC Server 330 Model 8640-EM2 (2 CPUs, PP-200)

IBM PC Server 330 Model 8640-ESS (2 CPUs, PP-200)

IBM PC Server 520 Model 8641-ED2 (2 CPUs, P-133)

IBM PC Server 520 Model 8641-EDG (2 CPUs, P-133)

IBM PC Server 520 Model 8641-EDV (2 CPUs, P-133)

IBM PC Server 520 Model 8641-EZ1 (2 CPUs, P-100)

IBM PC Server 520 Model 8641-EZE (2 CPUs, P-100)

IBM PC Server 520 Model 8641-EZO (2 CPUs, P-100)

IBM PC Server 520 Model 8641-EZS (2 CPUs, P-100)

IBM PC Server 520 Model 8641-EZV (2 CPUs, P-100)

IBM PC Server 520 Model 8641-MDV (2 CPUs, P-133)

IBM PC Server 520 Model 8641-MZE (2 CPUs, P-100)

IBM PC Server 520 Model 8641-MZL (2 CPUs, P-100)

IBM PC Server 520 Model 8641-MZO (2 CPUs, P-100)

IBM PC Server 520 Model 8641-MZS (2 CPUs, P-100)

IBM PC Server 520 Model 8641-MZV (2 CPUs, P-100)

IBM PC Server 704 Model 8650-6MM (4 CPUs, PP-200)

IBM PC Server 704 Model 8650-12U (4 CPUs, PP-166)

IBM PC Server 720 Model 8642-1ZO (2 CPUs, P-100)

IBM PC Server 720 Model 8642-4ZS (2 CPUs, P-100)

IBM PC Server 720 Model 8642-OZO (2 CPUs, P-100)

IBM Personal Computer 300 Model 6589-12U (2 CPUs, PP-200)

Intel Advanced EV Endeavour (2 CPUs, P-166)

Intel ALTserver Altair (2 CPUs, P-100)

Intel AP450GX MP Server (4 CPUs, PP-166)

Intel AP450GX MP Server (4 CPUs, PP-200)

Intel BB440FX Server (Buckeye) (2 CPUs, PP-200)

Intel BC440FX DP Server (2 CPUs, PP-200)

Intel DPServer R440LX (2 CPUs, PII-300)

Intel Express (4 CPUs, P-100)Hardware Compatibility List for Solaris 2.6 (Intel Platform Edition)39

TABLE

1{2Multiprocessor Systems (SMP)(continued)

Intel

Express Dual Pentium 60 (2 CPUs)

Intel Express Dual Pentium 66 (2 CPUs)

Intel OEM Xtended Xpress (4 CPUs, P-100)

Intel PR440FX (2 CPUs, PP-180)

Intel Xtended Xpress Server (2 CPUs, P-133)

Intel Xtended Xpress Server (2 CPUs, P-166)

Intel Xtended Xpress Server (4 CPUs, P-166)

Intergraph ISP32 (2 CPUs, P-90)

Intergraph ISMP22 (2 CPUs, P-90)

Intergraph ISMP32 (2 CPUs, P-90)

Intergraph ISMP6 (6 CPUs, P-100)

Intergraph ISMP620 (2 CPUs, PP-150)

Intergraph ISMP640 (4 CPUs, PP-200)

Intergraph TD-4 (2 CPUs, P-90)

Intergraph TD-4 (2 CPUs, P-100)

Intergraph TD-30 (2 CPUs, P-100)

Intergraph TD-40 (2 CPUs, P-100)

Intergraph TD-400 (2 CPUs, PP-150)

Intergraph TD-410 (2 CPUs, PP-200)

Intergraph TD-420 (2 CPUs, PP-200)

Intergraph TD-425 (2 CPUs, Pentium II-266)

Intergraph TD-5 (2 CPUs, P-90)

Micron Millennia Pro2-400-Plus (2 CPUs, PP-200)

Micron PowerServer SMP P-266 (2 CPUs, P-133)

Micron V etix 2LXI (2 CPUs, PP-200)

Micron V etix 2MXI (2 CPUs, PP-200)

Micron V etix EL 2000 (2 CPUs, PP-200)

Micron V etix EL 2000 IDE V ersion (2 CPUs, PP-200)

Mitsubishi Electric FT2200 (2 CPUs, PP-200+RAID)

Mitsubishi Electric FT4200 (2 CPUs, PP-200+RAID)

Mitsubishi Electric FT4200 (4 CPUs, PP-200)40

Hardware

Compatibility List for Solaris 2.6 (Intel Platform Edition)¤ January 1998

TABLE

1{2Multiprocessor Systems (SMP)(continued)

NCR S26 2CPU (2 CPUs, PP-166 512K)

NCR S26 2CPU (2 CPUs, PP-200 512K)

NCR S26 2CPU (2 CPUs, PII-300 512K)

NCR WorldMark 4300 2CPU (2 CPUs, PP-200 512K)

NCR WorldMark 4300 4CPU (4 CPUs, PP-166)

NCR WorldMark 4300 4CPU (4 CPUs, PP-200 512K)

NCR WorldMark 4300 4CPU (4 CPUs, PP-200 1 MB)

NCR WorldMark 4300 Rack 2NODE 4CPU(4 CPUs, PP-200 512K)

NEC Express5800-LE2200 (2 CPUs, PII-300)

NEC Express5800-MH4000 (2 CPUs, PP-200)

NEC Express5800-RM4100 (2 CPUs, PP-200)

Olivetti NETSTRADA 5000 Pro 200 Dual (2 CPUs, PP-200+RAID)

Olivetti NETSTRADA 7000 Pro 200 Quad (4 CPUs, PP-200)

Olivetti SNX-160MP (2 CPUs, P-90)

Olivetti SNX-400RS (4 CPUs, P-133)

OMEGABYTE SolarSERVER XPR180/D (2 CPUs, PP-180)

OMEGABYTE SolarSERVER XPR200/D (2 CPUs, PP-200)

Peacock AG LAN Server Model SSE 8332 (Dual Pentium 66 Intel Express)

Samsung Magic Power SPC 8500-P (2 CPUs, P-90)

Samsung Magic Power SPC 8500-P (2 CPUs, P-100)

Samsung Magic Power SPC 8500-P (2 CPUs, P-133)

Samsung SmartNet Server Model 625 (2 CPUs, PP-200)

Samsung SmartNet Server Model 645 (4 CPUs, PP-200)

Samsung Smart Station 620 (2 CPUs, PP-180)

Samsung SWS 520/90 (2 CPUs, P-90)

Samsung SWS 520/100 (2 CPUs, P-100)

Samsung SWS 520/133 (2 CPUs, P-133)HardwareCompatibility List for Solaris 2.6 (Intel Platform Edition)41

TABLE

1{2Multiprocessor Systems (SMP)(continued)

Siemens

Nixdorf AG PCD-5T (2 CPUs, P-100)

Siemens Nixdorf AG PCE-5Smp (4 CPUs, P-133)

Siemens Nixdorf AG PRIMERGY 350 (2 CPUs, P-90)

Siemens Nixdorf AG PRIMERGY 351 (2 CPUs, P-133)

Siemens Nixdorf AG PRIMERGY 360 (2 CPUs, PP-200)

Siemens Nixdorf AG PRIMERGY 550 (2 CPUs, P-133)

Siemens Nixdorf AG PRIMERGY 551 (2 CPUs, P-200)

Siemens Nixdorf AG PRIMERGY 560 (4 CPUs, PP-200)

Siemens Nixdorf AG PRIMERGY 561 (2 CPUs, PP-200)

Siemens Nixdorf PCD-5T/PCI90de (2 CPUs, P-90)

Siemens Nixdorf PCE-5Smp (4 CPUs, P-100)

Siemens Nixdorf PCE-5Smp (4 CPUs, P-133)

Toshiba SV3000 100HM (2 CPUs, P-100)

Tricord PowerFrame Enterprise Server ES3000 (4 CPUs)7

Tricord PowerFrame Enterprise Server ES4000 (6 CPUs) 7 Tricord PowerFrame Enterprise Server ES5000 (6 CPUs) 7 Tulip Vision Line TR6-SMP2 (2 CPUs, PP-200) 8 Unisys 5400 (2 CPUs, P-100)

Unisys 6000/500 Model 20 (2 CPUs) 9

Unisys Model SFE (4 CPUs, PP-166)

Unisys Model SVD-II (2 CPUs, P-166)

Viglen ProPenta Server (4 CPUs, PP-200)

Viglen LX Server Pro (2 CPUs, PP-200)

Viglen XX Pro Server (2 CPUs, PP-200)

Viglen XX Server-ZX (2 CPUs, P-100)42Hardware

Compatibility List for Solaris 2.6 (Intel Platform Edition)¤ January 1998

TABLE

1{2Multiprocessor Systems (SMP)(continued)

Wyse

Series 7000i, Model 760MP (4 CPUs)

Wyse 7000-760MP DX2-66 (3 CPUs)

Wyse 7000-765MP P66 (2 CPUs)

Zenith Data Systems Express5800-LE2200 (2 CPUs, PII-300)

Zenith Data Systems Express5800-MH4000 (2 CPUs, PP-200)

Zenith Data Systems Express5800-RM4100 (2 CPUs, PP-200)

Zenith Data Systems Z-Server EX DP66E Model 1000 (2 CPUs)

Zenith Data Systems Z-Server MX Dual P-133 (2 CPUs, P-133)

Zenith Data Systems Z-Server MX Dual P-166 (2 CPUs, P-166)

Zenith Data Systems Z-Server MX Quad P-166 (4 CPUs, P-166)

Zenith Data Systems Z-Server WG P90 (2 CPUs, P-90) 1.

Only tested in VGA mode due to integrated video memory size.

2. Additional con�guration is required to install the Solaris 2.6 software on this system; refer to the

notes on \Memory Mapping Problems" in Solaris 2.6 (Intel Platform Edition) Release Notes for

information.

3. Before installing the Solaris software on a ProLiant 5000, you must run the EISA con�guration utility

that came with your computer to enable APIC mode. For additional information, call your vendor’s

technical support number.

4. Refer to the certi�cation report for this system athttp://access1.sun.com/certify/reports/DEC/.

5. Must use a CD-ROM drive supported by the Solaris 2.6 operating environment.

6. Some versions may require a future Driver Update to support integrated video due to a

manufacturer’s part change.

7. Requires custom Solaris boot diskette to be supplied by Tricord.

8. For Solaris compatibility, specify an STB S3 Trio video system by requesting option

TR-16-200-4.0W-SFC4-P64/IS-4P41-U at time of order.

9. Must upgrade the system BIOS to V3.03.HardwareCompatibility List for Solaris 2.6 (Intel Platform Edition)43

TABLE

1{3Notebook Computers (Prior to March 1996) The following notebook computers have been certi�ed for standard Solaris

operation. Although some speci�c portable/nomadic computing capabilities have

been provided in the Solaris product, not all of the features and devices found on

these notebooks are currently supported. Many of these notebooks were tested

prior to the development of the formal notebook test plan now in use, so some

functionality may be limited. For additional information on using notebooks with

the Solaris product, see the online documentSolaris 2.5 x86 Notebook Supplement

Guide, part number 802-5028-10 (available through the Internet and other locations;

call your Sun Software Support Provider). Note that installation (booting) using

PCMCIA (PC Card) devices is not currently supported.

Ambra SN425C1

AST Ascentia 800N 486SX/33

AST Ascentia 900N 4/50

AST Ascentia 900N 4/75

AST Ascentia 910N (486DX2-50)

AST Power Exec 4/33 ColorPlus

Compaq LTE 4/25C

Compaq LTE 4/33

Compaq LTE Elite

Dell Latitude XP (DX4-100)

Ergo Powerbrick PN312/TFT (486DX4-100)

Everex StepNote (486DX4-100)

Fujitsu FMV-450NL/S (SL DX2-50)

Fujitsu FMV-5120 NAW

Gateway 2000 ColorBook 486DX4-75

IBM Model 755cx TFT Video (P-75)

IBM ThinkPad 750

IBM ThinkPad 750C

IBM ThinkPad 755C DX2/50

NEC V ersa/33

NEC V ersa/50

NEC V ersa/P44

Hardware

Compatibility List for Solaris 2.6 (Intel Platform Edition)¤ January 1998

TABLE

1{3Notebook Computers (Prior to March 1996)(continued)

Panasonic

CF-V21P

SiO Technologies FT-500 DX2/66

Tadpole 1000

Texas Instruments 4000E

Texas Instruments 5000

Toshiba 2400CT

Toshiba T1950CT

Toshiba T34002

Toshiba T3600

Toshiba T4400C 3 Toshiba T4600 3 Toshiba T4700C 3 Toshiba T4850CT (486DX4-100)

Toshiba T4800 2 Toshiba T4900CT (P-75) 4

Toshiba DynaBook SS475 051CT (486DX4-75)

Toshiba DynaBook SS475-JP

Toshiba Portege 610CT

Toshiba Satellite Pro T2150CDT (486DX4-75) 4 Toshiba Satellite Pro T2450CT (486DX4-75) 4 Twinhead Slimnote II (486E)

Zenith Data Systems Z-Note

Zenith Data Systems Z-Note ex

1. Keyboard controller problem affects installation. Refer to the patch �le included in theSUNWrdm

package located on the Solaris CD.

2. Requires special con�guration to install Solaris; only comes with a 120-Mbyte disk.

3. Some hardware con�guration may be required to install the Solaris software.

4. CAUTION: Some third-party memory expansion (PC Card) has been found to fail with the Solaris

operating environment. Use actual Toshiba or high-grade third-party memory.Hardware

Compatibility List for Solaris 2.6 (Intel Platform Edition)45

Notebook

Computers Certi�ed After March

1996

A test plan for notebook computers that more accurately represents the

status and support of a given model is now used.

The following matrix isnot intended to show which features a particular

notebook model has, but rather, which of the listed features currently works

with Solaris Intel Platform Edition. Models listed in the previous table, T able

1{3, have been tested for basic compatibility , but will not be retested to

provide the more speci�c information given in the table below .

For more detail, see the test reports onhttp://access1.sun.com/certify/reports/reports.html. For

additional information on video support, see T able 1{30 at the end of this

document.

TABLE

1{4Notebook Certi�cation Matrix (After March 1996) X mark or letters in a

box=Supported

DS=Dual scan

Int or Ext=Internal or external

NT=Not tested

NS=Not supported at this time

N/A=Not applicable

TFT=Active matrix

Manufacturer/

Model

CPU CD-

ROM

Int/Ext

Audio Modem

Int/PC

Card Display

Type

TFT/DS T ested

Display

Resolution

Dock

Bay Port

Repli-

cator Net-

work

1 Compaq

ARMADA 4120

P-120

Int

X

PC Cd

TFT

800x600

NT

NT

X LTE 5250

P-120

NT

X

PC Cd

TFT

800x600

NT

NT

X

Fujitsu

LifeBook 555Tx

P-150

MMX

Int

X

PC Cd

TFT

800x600

N/A

N/A

X LifeBook 655Tx

P-150

MMX

Ext

X

Int

TFT

800x600

N/A

X

X 46

Hardware

Compatibility List for Solaris 2.6 (Intel Platform Edition)¤ January 1998

TABLE

1{4Notebook Certi�cation Matrix (After March 1996)(continued) X mark or letters in a

box=Supported

DS=Dual scan

Int or Ext=Internal or external

NT=Not tested

NS=Not supported at this time

N/A=Not applicable

TFT=Active matrix

Manufacturer/

Model

CPU CD-

ROM

Int/Ext

Audio Modem

Int/PC

Card Display

Type

TFT/DS T ested

Display

Resolution

Dock

Bay Port

Repli-

cator Net-

work

1 IBM

ThinkPad 760CD

P-90

N/A

NS

Int/NS

TFT

800x600

NT

NT

X ThinkPad 760ED

P-133

N/A

NS

Int/NS

TFT

800x600

NT

NT

X

HP

Omnibook 5500CT

P-133

N/A

NS

PC Cd

TFT

800x600

NT

NT

X

Toshiba

Portege 650CT

P-133

N/A

NS

Int

TFT

800x600

NT

NT

X Satellite Pro

420CDT

P-100

Int

X

N/A

TFT

800x600

NT

NT

X Satellite Pro

425CDT

P-100

Int

X

N/A

TFT

800x600

NT

NT

X Tecra 500CDT

P-120

Int

NS

Int

TFT

800x600

NT

NT

X Tecra 720CDT

P-133

Int

NS

Int

TFT

1024x768

NT

NT

X Tecra 730CDT

P-150

Int

NS

Int

TFT

1024x768

NT

NT

X Tecra 700CT

P-120

Int

X

PC Cd

TFT

800x600

NT

N/A

X 1. Tested with 3Com EtherLink PC Card (PCMCIA) 3C589.Hardware Compatibility List for Solaris 2.6 (Intel Platform Edition)47

Supported DevicesDevices listed in this section have been successfully tested with Solaris 2.6Intel

Platform Edition in a varied but limited number of hardware

con�gurations. While a complete system composed of the devices listed in

this section should enable you to install and run the Solaris software, some

combinations of devices may not be usable or may require additional

con�guration. Note

- Devices that require additional con�guration and that have a Device

Reference Page in Device Reference Pages for Solaris 2.6 (Intel Platform

Edition) are marked with a # symbol. 48

Hardware

Compatibility List for Solaris 2.6 (Intel Platform Edition)¤ January 1998

TABLE

1{5SCSI Host Bus Adapters V endor Model Acculogic

PCIpport Model 20

Adaptec AHA-1510A#AHA-1520A # AHA-1522A # AHA-1530P/1532P # AHA-1540B/1542B # AHA-1540C/1542C # AHA-1540CF/1542CF # AHA-1540CP/1542CP # AHA-1640/1642 # AHA-1740/1742A # AHA-2740/2742 # AHA-2740A/2742A # AHA-2740T/2742T # AHA-2740AT/2742AT # AHA-2740W/2742W # AHA-2840A/2842A

AHA-2840VL/2842VL # AHA-2940/2940W # AHA-2940AU

AHA-2940U/2940UW # AHA-2944UW

AHA-2944W

AHA-3940/3940W # AHA-3940U/3940UW # AIC-6260

AIC-6360 # AIC-7770, AIC-7770 Rev . E

#Hardware

Compatibility List for Solaris 2.6 (Intel Platform Edition)49

TABLE

1{5SCSI Host Bus Adapters(continued) V endor Model Adaptec, cont.

AIC-7850

# AIC-7860 # AIC-7870 # AIC-7880 # APA-348 MiniSCSI (LPT/SCSI)

AMD PCscsi # PCscsi II # PCnet-SCSI #50

Hardware

Compatibility List for Solaris 2.6 (Intel Platform Edition)¤ January 1998

TABLE

1{5SCSI Host Bus Adapters(continued) V endor Model BusLogic

BT-440C (VLB)#

BT-445C (VLB) # BT-445S (VLB) # BT-542B (ISA) # BT-545C (ISA) # BT-545S (ISA) # BT-742A (EISA) # BT-746C (EISA) # BT-747C (EISA) # BT-747S (EISA) # BT-757C (EISA) # BT-757CD (EISA)

BT-757S (EISA) # BT-946C (PCI) # BT-948 (PCI)

BT-956C (PCI) # BT-956CD (PCI)

BT-958 (PCI)

BT-958D (PCI)

FlashPoint DL Dual-Channel Ultra SCSI (BT-932) (PCI) # FlashPoint DW Dual-Channel Ultra & Wide SCSI

(BT-952) (PCI) # FlashPoint LT Ultra SCSI (BT-930) (PCI) # FlashPoint LW Ultra & Wide SCSI (BT-950) (PCI)

#Hardware

Compatibility List for Solaris 2.6 (Intel Platform Edition)51

TABLE

1{5SCSI Host Bus Adapters(continued) V endor Model Compaq

32-bit Fast-SCSI-2 # 32-bit Fast-Wide SCSI-2/E # 32-bit Fast-Wide SCSI-2/P # Integrated 32-bit Fast-SCSI-2 # Integrated 32-bit Fast-SCSI{2/P # Integrated 32-bit Fast-Wide SCSI-2/E # Integrated 32-bit Fast-Wide SCSI-2/P # Integrated Wide-Ultra SCSI Controller (PCI) # Wide-Ultra SCSI Controller (PCI) # Creative Labs Sound Blaster 16 SCSI-2 #52

Hardware

Compatibility List for Solaris 2.6 (Intel Platform Edition)¤ January 1998

TABLE

1{5SCSI Host Bus Adapters(continued) V endor Model DPT

PM-2011 (EISA)#

PM-2012B (EISA) # PM-2021 (ISA) 1 # PM-2022 (EISA) 1 # PM-2024 (PCI) 1 # PM-2041 (ISA) 1 PM-2041W (ISA) 1 # PM-2042 (EISA) 1 PM-2042W (EISA) 1 # PM-2044UW (PCI) 1 # PM-2044W (PCI) 1 # PM-2122 (EISA) 1 # PM-2124 (PCI) 1 # PM-2124W (PCI) 1 # PM-2142W (EISA) 1 # PM-2144UW (PCI) 1 # PM-2144W (PCI) 1 # PM-3021 (ISA) # DTC DTC-3130 (PCI) 2

DTC-3130B (PCI)

Hitachi PC-CS7210 (PCI)

IBM PS/2 Micro Channel SCSI # SCSI-2 Fast/Wide Adapter/A # Intel PCISCSI (NCR 53C825) 3 # PCISCSINR (NCR 53C810) # P .E. Logic Corp PEL-16204HardwareCompatibility List for Solaris 2.6 (Intel Platform Edition)53

TABLE

1{5SCSI Host Bus Adapters(continued) V endor Model QLogic

QLA510 # Siemens Nixdorf PCE-5S (NCR 53C710) # Symbios Logic (also NCR) NCR 53C810 # NCR 53C810A # NCR 53C815 # NCR 53C820 3# NCR 53C825 3# NCR 53C825A 3# Trantor T348 MiniSCSI Plus Parallel # Tricord Intelligent SCSI Subsystem Controller # 1. This adapter can be made RAID-capable with the addition of a Hardware Disk Array module.

2. This adapter does not have the SDMS BIOS on board. It should be used only on a system that

contains the SCSI BIOS as part of its main system BIOS.

3. Wide SCSI not yet supported in Solaris driver.

4. Con�gure as an Adaptec AHA-1520A. Note

-Devices that require additional con�guration and that have a Device

Reference Page inDevice Reference Pages for Solaris 2.6 (Intel Platform

Edition) are marked with a # symbol.

Note - Entries marked with an asterisk (*) are newly supported and require

a Driver Update for proper operation.

TABLE 1{6 SCSI RAID Controllers

V endor Model

AMI MegaRAID 428 (PCI)

# *54

Hardware

Compatibility List for Solaris 2.6 (Intel Platform Edition)¤ January 1998

TABLE

1{6SCSI RAID Controllers(continued) V endor Model Compaq

SMART Array Controller#

SMART-2 EISA/PCI Array Controller # SMART-2DH Array Controller # SMART-2SL Array Controller # DEC Digital Storage Works RAID Array (EISA)

Dell PowerEdge RAID Controller II (PERC II) (PCI) * DPT PM-2044UW (PCI)

PM-2144UW (PCI)

PM-3222 (EISA) # PM-3222UW (EISA) # PM-3224 (PCI) # PM-3224W (PCI) # PM-3332UW (EISA) # PM-3334UW (PCI) # PM-3334W (PCI) # HP HP Disk Array/HP Disk SystemHardware

Compatibility List for Solaris 2.6 (Intel Platform Edition)55

TABLE

1{6SCSI RAID Controllers(continued) V endor Model IBM

PC ServeRAID Adapter (Copperhead) (PCI)#

SCSI-2 RAID Controller (MCA) # SCSI-2 Fast/Wide Streaming RAID Adapter

(MCA) # SCSI-2 Fast/Wide RAID Adapter (PCI)

Mylex DAC960E (EISA) # DAC960M (Micro Channel)

DAC960P (PCI) # DAC960PD (PCI) # DAC960PD-Ultra (PCI) # DAC960PL (PCI) # TABLE 1{7 Solid State SCSI Disk Devices

V endor Model

ATTO Technology Silicon Disk II (SCSI F/W)

Imperial Technology MegaRam (268 MB version) 56

Hardware

Compatibility List for Solaris 2.6 (Intel Platform Edition)¤ January 1998

TABLE

1{8CD-ROM Drives V endor Model Type Chinon

CDS435

CDS-525

CDS535

1 SCSI

SCSI

SCSI

GoldStar CRD-8160B 16x

GCD-R320B

GCD-R520B

GCD-R580B 8x ATAPI/IDE

SCSI

ATAPI/IDE

ATAPI/IDE

Hitachi CDR-1900S

CDR-3750

CDR-6750

CDR-7730

CDR-7930 8x

CDR-8130 16x

MaxPC-UC5240 4x SCSI

SCSI

SCSI

ATAPI/IDE

ATAPI/IDE

ATAPI/IDE

SCSI

Lion Optics XC200SI SCSI

LMSI CM214

CM215

SCSI

Mitsumi CRMC-FX001DE

CRMC-FX400

ATAPI/IDE

ATAPI/IDE

NEC CDR-2102

SCSI

CDR-211 SCSI

CDR-250 ATAPI/IDE

CDR-260 ATAPI/IDE

CDR-260R ATAPI/IDE

CDR-271 ATAPI/IDE

CDR-272 (4x speed) ATAPI/IDE

CDR-272 Rev . 4.15 ATAPI/IDEHardware

Compatibility List for Solaris 2.6 (Intel Platform Edition)57

TABLE

1{8CD-ROM Drives(continued) V endor Model Type CDR-273

(6x speed) ATAPI/IDE

CDR-280 ATAPI/IDE

CDR-510 SCSI

CDR-1400 (8x speed) ATAPI/IDE

CDR-1400A (8x speed) SCSI-2

CDR-1410A (8x speed) SCSI-2

CDR-1600A (12/16x

speed)

ATAPI/IDE

CDR-1610A (12/16x

speed)

SCSI

CDR-1610A (12/16x

speed)

ATAPI/IDE

Intersect CDR-74 SCSI

Intersect CDR-84 SCSI

MultiSpin 2Vi ATAPI/IDE

MultiSpin 3Xe2 SCSI

MultiSpin 3Xi

2 SCSI

MultiSpin 3Xp Plus SCSI

MultiSpin 4Xe

1 2 SCSI

MultiSpin 4Xi

1 2 SCSI

MultiSpin 6Xi SCSI

Optics Storage 8422IDE ATAPI/IDE58

Hardware

Compatibility List for Solaris 2.6 (Intel Platform Edition)¤ January 1998

TABLE

1{8CD-ROM Drives(continued) V endor Model Type Panasonic

LK-MC509S

LK-MC579B

LK-MC608B 8x

LK-MC688B 8x SCSI

ATAPI/IDE

SCSI

ATAPI/IDE

Panasonic/Matsushita CR-504B 4x

CR-572B

SCSI

ATAPI/IDE

Philips CM207

CM215

CM425A ATAPI/IDE

SCSI

SCSI

Pioneer DR-U12X (12x speed) SCSI

DRM-604X 1 3 SCSI

DRM-624X

1 3 SCSI

Plextor DM3028

PX-12CSi

PX-12TSi

PX-20TSi

PX-43CE (4.5 Plex)

PX-43CH (4 Plex)

PX-43CS

PX-45CH

PX-45CS

PX-63CS (6 Plex)

PX-65CS (6 Plex)

PX-83CS (8 Plex) SCSI

SCSI

SCSI

SCSI

SCSI

SCSI

SCSI

SCSI

SCSI

SCSI

SCSI

SCSI

Reveal 4X Internal ATAPI/IDE

Sanyo CRD-254P

CDR-H93RMV

CDR-400I ATAPI/IDE

SCSI

SCSI

Hardware

Compatibility List for Solaris 2.6 (Intel Platform Edition)59

TABLE

1{8CD-ROM Drives(continued) V endor Model Type Sanyo-TORiSAN

CDR-S1G

CDR-S18

ATAPI/IDE

ATAPI/IDE

Sony CDU-55E ATAPI/IDE

CDU-55S

4 SCSI

CDU-561 SCSI

CDU-76E ATAPI/IDE

CDU-76S SCSI

CDU-77E ATAPI/IDE

CDU-6211 SCSI

CDU-6811 SCSI

CDU-7211 SCSI

CDU-7811 SCSI

CDU-8012 SCSI

Sun Microsystems SunCD SCSI

Tae I1 Media Co. TechMedia CDD-6100 10X ATAPI/IDE

TEAC CD-56E ATAPI/IDE

Texel DM3024

DM3028

DM5021

DM5024

DM5028 SCSI

SCSI

SCSI

SCSI

SCSI 60

Hardware

Compatibility List for Solaris 2.6 (Intel Platform Edition)¤ January 1998

TABLE

1{8CD-ROM Drives(continued) V endor Model Type Toshiba

4101-TA

5201B

TXM-3201

TXM-3301

TXM-3401

TXM-3701-D1

XM-3501B

XM-3601B

XM-5302B

XM-5522B

XM-5602B (8x)

XM-5701TA (12x)

XM-5702B (12x) SCSI

SCSI

SCSI

SCSI

SCSI

SCSI

SCSI

SCSI

ATAPI/IDE

ATAPI/IDE

ATAPI/IDE

SCSI

ATAPI/IDE

Wearnes CDD-1205 ATAPI/IDE

1. Various CD-ROM players may not be fully SCSI-compliant in their handling of theCDROMREADHEADER command. This may cause failures from vold not mounting an eligible

CD-ROM. The workaround is to mount the CD-ROM manually.

2. Early versions of NEC �rmware were not fully SCSI-compliant; thus these drives may only work if

synchronous negotiation and disconnect are disabled on the SCSI adapter used with the CD-ROM

drive, or if the drive is jumpered to use scsi-1 commands, as appropriate.

3. Only the �rst CD-ROM in the Pioneer DRM-604X CD-ROM changer is supported by default.

4. This drive does not work with the Adaptec AHA-2940 SCSI HBA.

5. Must have BIOS 1.0 or later.Hardware Compatibility List for Solaris 2.6 (Intel Platform Edition)61

TABLE

1{9Printing Devices V endor Model Lexmark

International Optra C color laser printer

Optra N network laser printer

Optra R+ laser printer

Optra Rt+ laser printer

Optra Lx+ laser printer

Optra Lxi+ laser printer

Color Jetprinter PS 4079 plus printer Note

-Devices that require additional con�guration and that have a Device

Reference Page inDevice Reference Pages for Solaris 2.6 (Intel Platform

Edition) are marked with a # symbol.

TABLE 1{10 Audio Devices

V endor Model

Analog Devices AD1848 & compatibles#

Compaq Business Audio62

Hardware

Compatibility List for Solaris 2.6 (Intel Platform Edition)¤ January 1998

TABLE

1{10

Audio Devices(continued) V endor Model Creative

Labs Sound Blaster 16#

Sound Blaster 16 SCSI-2 # Sound Blaster AWE32 # Sound Blaster Pro # Sound Blaster Pro{2 # Sound Blaster Vibra 16 # Various Other Boards and

Devices

Drivers and support for a large number of additional

sound boards and devices are available using a

software driver package from 4Front Technologies. To

obtain it, contact the vendor:

Tel: (310) 820-7365 USA

Fax: (310) 826-2465 USA

Email:

info@4front-tech.com

Web: http://www.4front-tech.com

TABLE 1{11 Telephony Products

V endor Model Description

Dialogic

Corporation 1

D/21D 2 POTS lines voice and tone recognition

D/41D 4 POTS lines voice and tone recognition

D/41E 4 POTS lines

D/121A 12{port voice and tone recognition, and processing

board

D/121B 12{port voice and tone recognition, and processing

board

D/240SC 24-channel voice store and forwardHardware

Compatibility List for Solaris 2.6 (Intel Platform Edition)63

TABLE

1{11

Telephony Products(continued) V endor Model Description D/320SC

32{channel voice store and forward

D/240SC-T1 32{channel voice store and forward, with T-1

FAX/40 Fax daughtercard, 4 channel, for D/41

FAX/120 12{channel Fax for D/121 boards

VR/40 Multiline speech recognition daughterboard, 4 port

VR/121 Multiline speech recognition daughterboard, 12 port

VR/160 Multiline speech recognition daughtercard, 16 port

VR/160C Multiline speech recognition daughtercard, 16 port

DTI/211 Digital Trunk Interface, North American T-1

DTI/212 Digital Trunk Interface, European E-1

LSI/120 Loop Start Interface board

LSI/180 Loop Start Interface board

DMX Digital Multiplexor Expansion boards

MSI Modular Station Interface board, 24 port 1.

Device driver software and support are supplied by the vendor.

TABLE 1{12 Multiport Serial Adapters

V endor Model

Aurora

1 401A (ISA 4 Port)

Aries 8000P (PCI 8 Port)

Aries 1600P (PCI 16 Port)

CHASE 1 IOPRO (ISA 8 Port)64

Hardware

Compatibility List for Solaris 2.6 (Intel Platform Edition)¤ January 1998

TABLE

1{12

Multiport Serial Adapters(continued) V endor Model COMPUTONE1 IntelliServer SVR-16DB (16 Port)

COMTROL

1 Rocketport (16 Port) Digi International

(DigiBoard) 1

AccelePort (ISA)

C/X Intelligent Clusters (ISA, EISA)

EPC/X Intelligent Clusters (ISA, EISA)

PC/8e (ISA)

PC/8eV e

PC/16em (16 db25 port)

PC/Xe Intelligent Serial Adapters

PC/Xem (ISA, EISA)

PC/Xi Intelligent Serial Adapters

PCI/8r (PCI)

PCI/16em (16 db25 port)

PCI/Xem

Xem Intelligent Asynchronous Adapters

Xr Intelligent Asynchronous Adapters

MILAN

1 FastPort 3100CX PrintServer

FastPort 3200C PrintServer

FastPort 3400C PrintServer

Moxa

1 MOXA-C218 (ISA 8 Port)

MOXA-C320 (ISA 32 Port)

Specialix

1 SI/8 AT

XIO/8 AT

Stallion

1 EasyServer II Terminal Server Systech

1 Parallex SCS-2008I (ISA 8 Port)

RCS-4008 Network Terminal Server

RCS-4008 TCP Terminal Server 8-port

RCS-4108 TCP Terminal Server 8-port Hardware

Compatibility List for Solaris 2.6 (Intel Platform Edition)65

TABLE

1{12

Multiport Serial Adapters(continued)

1. Solaris drivers for this vendor’s devices are available directly from the vendor. Note

-Devices that require additional con�guration and that have a Device

Reference Page inDevice Reference Pages for Solaris 2.6 (Intel Platform

Edition) are marked with a # symbol.

Note - Entries marked with an asterisk (*) are newly supported and require

a Driver Update for proper operation.

TABLE 1{13 Network Adapters|Ethernet V endor Name/Model 3Com

EtherLink II, II/16 (3C503, 3C503-16) # EtherLink 16, 16TP (3C507, 3C507-TP) # EtherLink III (3C509, 3C509B 1 , 3C529, 3C59x) # EtherLink III PCMCIA (3C562, 3C589, 3C589B, 3C589C, 3C589D) # EtherLink III PCI Bus Master (3C590)

EtherLink III EISA Bus Master (3C592)

EtherLink XL (3C900-TPO, 3C900-COMBO) # Fast EtherLink 10/100 PCI (3C595 TX)

Fast EtherLink 10/100 EISA (3C597 TX)

Fast EtherLink XL (3C905) # Accton EN1625 (ISA)

EtherCombo-16 (ISA) 266

Hardware

Compatibility List for Solaris 2.6 (Intel Platform Edition)¤ January 1998

TABLE

1{13

Network Adapters|Ethernet

(continued) V endor Name/Model Adaptec

ANA-6901 (PCI)

ANA-6901/C (PCI)

ANA-6904 (PCI)

ANA-6911A/C (PCI)# *

ANA-6911A/TX (PCI) # * ANA-6911/TX (PCI)

ANA-6944A 10/100 TX 4-port (PCI)

Allied

Telesyn

AT-1500 (ISA) # AT-1500T-Plus (ISA)

AT-1500BT-Plus (ISA)

AT-2450 10 T (PCI)

AT-2560 10/100 TX (PCI)

Alta EtherCombo-16 T/C (ISA)2 3

AMD PCnet-ISA controller chip # PCnet-PCI controller chip # PCnet-PCI II controller chip #* Asante AsanteFAST 10/100 (PCI) 4 # Cabletron E-2210 (ISA) # * CNet CN970EBT (PCI)

PowerNIC CN935E (PCI) 4 # Cogent EM110 T4 (PCI)

4 # *

EM110TX (PCI) 4 # EM440 QUAD (PCI) 4 # EM960C (PCI)

4 5 #

EM960TP (PCI) 4 # EM964 QUAD (PCI)

4 #Hardware

Compatibility List for Solaris 2.6 (Intel Platform Edition)67

TABLE

1{13

Network Adapters|Ethernet

(continued) V endor Name/Model Compaq

Deskpro 4000 Integrated NetFlex-3 10/100#

Deskpro 6000 Integrated NetFlex-3 10/100 # Netelligent 10T PCI 6 # Netelligent 10/100 TX PCI 6 # NetFlex-2 DualPort ENET

NetFlex-2 ENET-TR Controller (Ethernet only)

NetFlex-3 DualPort 10/100TX PCI # NetFlex-3/E 6 # NetFlex-3/P 6 # Professional Workstation 5000 Integrated NetFlex-3 10/100 # ProLiant 800 Integrated NetFlex-3 10/100 # ProLiant 2500 Integrated NetFlex-3 10/100 # Compex ENET32-PCI

ReadyLINK ENET32 4 # DEC EtherWORKS 10/100 4 # EtherWORKS PCI 10/100 4 # Diversi�ed

Technologies

(DTI) LBC5025

4 5 #

D-Link DE-530CT (PCI) 4 # DE-530CT+ (PCI) 4 # DFE{500TX (Revision B1) (PCI)

Genius GE2000III (ISA)

HP PC LAN NC/16 TP J2405A

IBM IBM 100/10 PCI Ethernet Adapter

IBM LAN Adapter for Ethernet Combo (ISA)

IBM LAN Adapter for Ethernet CX (ISA)

IBM LAN Adapter for Ethernet TP (ISA)68

Hardware

Compatibility List for Solaris 2.6 (Intel Platform Edition)¤ January 1998

TABLE

1{13

Network Adapters|Ethernet

(continued) V endor Name/Model Intel

EtherExpress16 (PCLA8110)#

EtherExpress16 TP (PCLA8120) # EtherExpress16C (PCLA8100) # EtherExpress 32 (EILA8215) (EISA)

EtherExpress Flash32 (EILA8225A) (EISA) # EtherExpress FlashC (PCLA8105)

EtherExpress MCA (MCLA8110) # EtherExpress MCA TP (MCLA8120) # EtherExpress PRO (ISA) # EtherExpress PRO/10+ (ISA) # EtherExpress PRO/10+ (PILA8400/8420) (PCI)

EtherExpress PRO/100 (EILA8265F EISA) # EtherExpress PRO/100 (PILA8465) (PCI) # EtherExpress PRO/100B (82557) (PCI)

Kingston KNE40BT 4 # KNE100TX (PCI) 4 # KNE2000T+ (ISA) 3 KNE2002+ (ISA) 3 KNE2031+ (ISA) 3 KNE2121+ (ISA)

KNE2121H (ISA)

Linksys LNE100TX (PCI) 4 # LNEPCI (PCI)

Microdyne NE2000 (ISA) # NE2500plus (ISA) # Mitron LX2100p (PCI)Hardware Compatibility List for Solaris 2.6 (Intel Platform Edition)69

TABLE

1{13

Network Adapters|Ethernet

(continued) V endor Name/Model National

Semicond.

Infomover NE2000plus (ISA)3 #

NetGear FA310TX 10T/100TX (PCI)

Novell/

Eagle Tech.

NE2000 (ISA) # NE2000plus (ISA) 3 # NE3200 (EISA) # Olicom EtherCom ISA/II3

Racal

InterLan

ES3210/ES3210 TP Ethernet 7 # PCI T2-STR

Rockwell RNS 2300 4 # RNS 2340 QUAD

4 5 #

Samsung SEB-3000C (PCI)70

Hardware

Compatibility List for Solaris 2.6 (Intel Platform Edition)¤ January 1998

TABLE

1{13

Network Adapters|Ethernet

(continued) V endor Name/Model SMC

Dual Channel 10T/100TX (9334BDT) (PCI)

Elite32 (8033) (EISA)#

Elite32C Ultra (8232) (EISA) # Ether 10/100 (9232) (EISA) # EtherCard PLUS (8003) # EtherCard PLUS Elite (8013) # EtherCard PLUS Elite 16 (8013) # EtherCard Elite16 Ultra (8216) # EtherCard Elite 32T (8033) # EtherEZ (8416) # EtherPower 8432BT (PCI) 4 # EtherPower 8432BTA (PCI) 4 # EtherPower 8432T (PCI) 4 EtherPower 10/100 (9332BDT) (PCI) 4 # EtherPower 10/100 (9332DST) (PCI)

4 5 #

SVEC ETHER-100TX (PN 100TX 10/100TX) (PCI)

FD0421-P Rev . A-1 (ISA)

FD0455 EtherBoard-PCI

NE2100 (ISA)

Texas

Instru-

ments ThunderLAN 10/100 TX (PCI)

Thomas

Conrad

NE2000 (ISA)

Unisys EISA Ethernet controller (Intel 82596)

U6000/DT2 integrated Ethernet controller (Intel 82596)Hardware

Compatibility List for Solaris 2.6 (Intel Platform Edition)71

TABLE

1{13

Network Adapters|Ethernet

(continued) V endor Name/Model Xircom

Pocket Ethernet Adapter III (PE3)#

Znyx NetBlaster ZX314 QUAD 4 # NetBlaster ZX315 DUAL 4 # NetBlaster ZX345 4 # NetBlaster ZX346 QUAD

4 5 #

NetBlaster ZX348 DUAL 4 # ZX311 4 # ZX312 (PCI)

4 5 #

ZX342 10/100 (PCI)

4 5 #

ZX344 QUAD 4 # 1. Cards with \ASSY 03-0021-000, REV A" printed on them do not work with the Solaris software.

2. Card misdetects 8-bit slot.

3. Some NE2000plus clones may only work in I/O or shared memory mode, depending on the system

or con�guration, while running Solaris software.

4. Because certain board revisions have been found not to work, refer to the table in the \DEC 21040,

21041, 21140, 21142, 21143 Ethernet" Device Reference Page for additional information.

5. Special con�guration required; refer to the table in the \DEC 21040, 21041, 21140, 21142, 21143

Ethernet" Device Reference Page for additional information.

6. Refer to the \Compaq NetFlex-3, Netelligent Controllers" Device Reference Page.

7. Only the newer versions of these cards are supported. The versions successfully tested have stickers

with the numbers 625-0367-00 and 625-0369-00; older versions of the card, for example, those with

the number 625-0136-00, do not work. Note

-Devices that require additional con�guration and that have a Device

Reference Page inDevice Reference Pages for Solaris 2.6 (Intel Platform

Edition) are marked with a # symbol.

Note - Entries marked with an asterisk (*) are newly supported and require

a Driver Update for proper operation. 72

Hardware

Compatibility List for Solaris 2.6 (Intel Platform Edition)¤ January 1998

TABLE

1{14

Network Adapters|Fast Ethernet V endor Name/Model 3Com

Fast EtherLink 10/100 (3C595 TX) (PCI)

Fast EtherLink 10/100 (3C597 TX) (EISA)

Fast EtherLink XL (3C905)#

Adaptec ANA-6901 (PCI)

ANA-6901/C (PCI)

ANA-6904 (PCI)

ANA-6910/TX (PCI)

ANA-6911A/C (PCI) # * ANA-6911A/TX (PCI) # * ANA-6911/TX (PCI)

ANA-6940/TX (PCI)

ANA-6944A 10/100 TX 4-port (PCI)

Allied Telesyn AT-1500 (ISA) # AT-2560 10/100 TX (PCI)

AMD PCnet-Fast #* Asante AsanteFAST 10/100 (PCI) 1 # Cogent EM100 (PCI) 1 # EM100TX (PCI) 1 # EM110 T4 (PCI)

1 # *

EM110TX (PCI) 1 # EM400 QUAD (PCI) 1 # EM440 QUAD (PCI)

1 #Hardware

Compatibility List for Solaris 2.6 (Intel Platform Edition)73

TABLE

1{14

Network Adapters|Fast Ethernet(continued) V endor Name/Model Compaq

Deskpro 4000 Integrated NetFlex-3 10/100#

Deskpro 6000 Integrated NetFlex-3 10/100 # Netelligent 10/100 TX PCI 2 # NetFlex-3 DualPort 10/100TX PCI # NetFlex-3/E w/100Base-TX UTP Module,

w/100VG-AnyLAN UTP Module, w/100Base-FX Module # NetFlex-3/P w/100Base-TX UTP Module,

w/100VG-AnyLAN UTP Module, w/100Base-FX Module # Professional Workstation 5000 Integrated NetFlex-3 10/100 # ProLiant 800 Integrated NetFlex-3 10/100 # ProLiant 2500 Integrated NetFlex-3 10/100 # DEC EtherWORKS 10/100 1 # EtherWORKS PCI 10/100 1 # Diversi�ed

Technologies (DTI)

LBC5025

1 3 #

IBM IBM 100/10 PCI Ethernet Adapter

Intel EtherExpress PRO/100 (82556) # EtherExpress PRO/100B (82557) (PCI)

Kingston KNE-100TX (PCI) 1 # Linksys LNE100TX (PCI) 1 # NetGear FA310TX 10T/100TX (PCI)

Rockwell RNS 2300 1 # RNS 2340 QUAD

1 3 #74

Hardware

Compatibility List for Solaris 2.6 (Intel Platform Edition)¤ January 1998

TABLE

1{14

Network Adapters|Fast Ethernet(continued) V endor Name/Model SMC

Dual Channel 10T/100TX ( 9334BDT) (PCI)

Ether 10/100 (9232) (EISA)#

EtherPower 10/100 (9332BDT) (PCI) 1 # EtherPower 10/100 (9332DST) (PCI)

1 3 #

SVEC ETHER-100TX (PN 100TX 10/100TX) (PCI)

Texas Instruments ThunderLAN 10/100 TX (PCI)

Znyx NetBlaster ZX345 1 # NetBlaster ZX346 QUAD

1 3 #

NetBlaster ZX348 DUAL 1 # ZX342 10/100 (PCI)

1 3 #

ZX344 QUAD 1 # 1. Because certain board revisions have been found not to work, refer to the table in the \DEC 21040,

21041, 21140, 21142, 21143 Ethernet" Device Reference Page for tested part/version numbers and

chipsets.

2. Refer to the \Compaq NetFlex-3, Netelligent Controllers" Device Reference Page for tested chipsets.

3. Special con�guration required; refer to the \DEC 21040, 21041, 21140, 21142, 21143 Ethernet" Device

Reference Page for additional information. Note

-Entries marked with an asterisk (*) are newly supported and require

a Driver Update for proper operation. Hardware

Compatibility List for Solaris 2.6 (Intel Platform Edition)75

TABLE

1{15

Network Adapters|Token Ring V endor Name/Model3ComTokenLink III (3C619, 3C629, 3C679)

IBM Auto 16/4 Token Ring (ISA, MCA)#

Token Ring 16/4 Adapter/A

Turbo 16/4 Token Ring

Madge PCI Presto # * Smart 16/4 AT Plus # * Smart 16/4 AT PnP # * Smart 16/4 EISA # * Smart 16/4 ISA Client Plus # * Smart 16/4 ISA Client PnP # * Smart 16/4 PCI BM Mk1 # * Smart 16/4 PCI Mk2 # * TABLE 1{16 Network Adapters|WAN

V endor Name/Model

TSG (The Software Group) NetcomHighway/572 (PCI)1

1. Driver software and support for this device are available directly from the vendor.

TABLE 1{17 AT-ISDN Adapters

V endor Name/Model

Digi International 1 Digi Data�re-U

Digi Data�re S/T 76

Hardware

Compatibility List for Solaris 2.6 (Intel Platform Edition)¤ January 1998

TABLE

1{17

AT-ISDN Adapters(continued)

1. Driver software and support for these devices are available directly from the vendor.

TABLE 1{18 High-Speed Networking V endor Name/Model ADAX APC-EIX T-1 Network Interface Board

(EISA) 1 1. Driver software and support for this device are available directly from the vendor.

TABLE 1{19 PC Card (PCMCIA)|Add-On Boards

V endor Name/Model

ATI

Technologies

14400 ETC-EXPRESS AX/Data Modem

Hytec HCD 22

SanDisk Flash PC Card SCM

Microsys.

SwapBox Classic

SwapBox Premium

Viper 8260pA Hardware

Compatibility List for Solaris 2.6 (Intel Platform Edition)77

TABLE

1{20

PC Card (PCMCIA)|GPS and Navigation Devices V endor Name/Model Centennial

Technologies

SatNav GPS Card|NMEA1

SatNav GPS Card|Binary 1 1. Tested only at the device level. Application software is available from various third-party vendors.

TABLE 1{21 PC Card (PCMCIA)|Modems

V endor Name/Model

ActionTec MD28801 (V .34 Fax/Modem)

APEXData PCA-1414 (Data/Fax)

AT&T Paradyne 371-B1-001 (14.4 Data/Fax)

Boca-Modem m144pa (14.4bps V32bis Data/Fax)

Centennial Tech. PM50003 (CT 14.4 Fax/Modem)

Compaq SpeedPaq 192

DataRace RediCard V ersion 1 (V .32bis/V .42/V .42bis Fax/Data)

RediCard V ersion 2 (V .32bis/V .42/V .42bis Fax/Data)

Hayes 5361US (Accura 336 T2 + Fax) (33.6Kbps V .34)

Optima 144

IBM 24TTMOD-W14 (14.4 Data/Fax)

87G9800 (V .32bis/V .42/V .42bis Fax/Data)

Intel 110-US (2400 Data)

Kingston DataRex 87G9851 (V .32bis/V .42/V .42bis Fax/Data)78Hardware Compatibility List for Solaris 2.6 (Intel Platform Edition)¤ January 1998

TABLE

1{21

PC Card (PCMCIA)|Modems

(continued) V endor Name/Model Megahertz

CC3144 (V .32bis/V .42/V .42bis Fax/Data)

XJ114 (V .32bis/V .42/V .42bis Fax/Data)

XJ124FM (V .32bis/V .42/V .42bis Fax/Data)

XJ214 (V .32bis/V .42/V .42bis Fax/Data)

XJ2288 (V .32bis/V .42/V .42bis Fax/Data)

Motorola Montana 33.6 (V .34 Fax/Modem)

SMART Modular Tech. SmartExchange 9624 Fax/Modem

Supra COMcard 144 (V .32bis/V .42/V .42bis Fax/Data)

US Robotics Sun/USR WorldPort (V .32bis/V .42/V .42bis

Fax/Data/V oice)

TABLE 1{22 PC Card (PCMCIA)|Serial Cards

V endor Name/Model

IBM IBM RS-332 Serial Card

Socket Communication SL0700 (RS-332) Hardware

Compatibility List for Solaris 2.6 (Intel Platform Edition)79

TABLE

1{23

PC Card (PCMCIA)|SRAM Memory Cards V endor Name/Model Centennial

Technologies SRAM Card (256 KB)

SRAM Card (512 KB)

SRAM Card (1 MB)

SRAM Card (2 MB)

SR04M-15-11192-01 52795 (4 MB Recharge)

Epson NB70-004268

NB70-004269

NB70-004270

IBM 0.5 MB SRAM Card

1 MB SRAM Card

0933155 (2 MB SRAM)

Magic Ram SR1MBP100

SR2MBP100

Mitsubishi MF3513-LCDAT

MF31M1-LCDAT

MF32M1-LCDAT

SMART Modular Technologies SM9SRD512KP3

SM9SRD1MP3

SM9SRD2MP3

SM9SRDA1MP3

SM9SRDA2MP3 80

Hardware

Compatibility List for Solaris 2.6 (Intel Platform Edition)¤ January 1998

TABLE

1{24

Pointing Devices V endor Model Appoint Thumbelina

1MousePen Pro 1 CH Products RollerMouse

Dyna Point DynaTrak1

IBM PS/2 2-button

Easy Options Mouse 1 Interlink PortaPoint 1 Kraft Systems MicroTrack 1 Logitech C7 serial and bus mouse devices

C9 serial and bus mouse devices

2-Button 1 MouseMan serial and bus mouse devices

MouseMan cordless

TrackMan serial and bus mouse devices

Microsoft Serial, bus, and PS/2 mouse devices

MicroSpeed MicroTRAC trackball

Mouse Systems Mouse!

New Mouse

PC Mouse II

1. Select \Microsoft 2-button mouse" during installation of Solaris software. Note

-The tape drives in the following table have been tested with thest

tape driver software. The tape drives were tested using the Legato T ape

Exerciser program to verify basic functionality and general compatibility

with Solaris 2.6Intel Platform Edition. Hardware

Compatibility List for Solaris 2.6 (Intel Platform Edition)81

TABLE

1{25

Tape Drives|SCSI V endor Model Archive

2150S 150 MB

2525 QIC-525

4320 4mm

4324 4mm

Python 28454 4mm

Python 28388 4mm

Viper

Compaq DLT 4000

DLT 7000

Conner CTD 2004 4mm

CTD 4004 4mm

CTD 8004H 4mm

DEC DLT 2000

Exabyte EXB-4200 4mm

EXB-8200 8mm

EXB-8500 8mm

EXB-8505 8mm

EXB-8505XL 7/14GB 8mm

8705 Eliant 8mm

EXB{8900 Mammoth 20/40 GB 8mm82

Hardware

Compatibility List for Solaris 2.6 (Intel Platform Edition)¤ January 1998

TABLE

1{25

Tape Drives|SCSI(continued) V endor Model HP 1557A DDS3 autoloader1, 2

Colorado Memory Systems PowerTape 1100 QIC

Colorado Memory Systems PowerTape 2400 QIC

Colorado Memory Systems PowerTape 4000 QIC

Colorado Memory Systems PowerDAT

6000 4mm 2 35470A DDS 4mm

35480A DDS/Data Compression 4mm

C1528E 4mm

C1533-00100 DDS2/Data Compression 4mm

C1534A DDS Tape Drive 4mm

C1536A DDS/Data Compression 4mm

C1537 DDS3 4mm

C1520F SureStore Tape 2000e 4mm

C1525F SureStore Tape 2000i 4mm

C1521F SureStore Tape 5000e 4mm

C1526F SureStore Tape 5000i 4mm

C1551A SureStore Tape 5000eU 4mm

C1529F SureStore Tape 6000e 4mm

C1528F SureStore Tape 6000i 4mm

C1552A SureStore Tape 6000eU 4mm

C1520E JetStore 2000e 4mm

C1520E JetStore 2000i 4mm

C1526E JetStore 5000i 4mm

C1529A JetStore 5000i 4mm

JetStore 5000e 4mm

SureStore DAT8 2 SureStore DAT24 2 SureStore DAT24x6e

1, 2

SureStore T4Hardware

Compatibility List for Solaris 2.6 (Intel Platform Edition)83

TABLE

1{25

Tape Drives|SCSI(continued) V endor Model Quantum

DLT 4000

DLT 7000

Sony SDT 5000 4mm

SDT 5200 4mm

SDT 7000 DDS2

SDT 9000 DDS3

Sun Microsystems DLT drives, all shipping models up to DLT 7000

x660A 150 MB QIC

x814A 5.0 GB 8mm

x822A 4mm

x6101A 2.5 GB QIC SCSI

x6102A 2.5 GB QIC SCSI

x6103A 2.5 GB QIC SCSI

Tecmar TS-420

Tandberg Panther 525S

TDC 3820

TDC 4120

TDC 4220

TDC 4222

TDC 6122

WangDAT 3400DX DDS-2 4mm

3800 DDS-2 4mm

Wangtek 51000 QIC

52000 QIC

5525ES QIC

9500DC QIC 1.

Requires third-party software.

2. Testing has shown that these switch settings are best: Switches 1 through 8; set to 11001100.84

Hardware

Compatibility List for Solaris 2.6 (Intel Platform Edition)¤ January 1998

TABLE

1{26

SCSI RAID Tape V endor Model ANDATACO

Rapid Tape Array

TABLE 1{27 Uninterruptable Power Supplies (UPS)

The following UPS products have been tested in the vendor’s labs. SunSoft has tested the

software on selected models to ensure basic operation under Solaris 2.6Intel Platform Edition.

APC Back-UPS 200

APC Back-UPS 280

APC Back-UPS 400

APC Back-UPS 450

APC Back-UPS 600

APC Back-UPS 900

APC Back-UPS 1250

APC Back-UPS Pro 280

APC Back-UPS Pro 420

APC Back-UPS Pro 650

APC Back-UPS Pro 1000

APC Back-UPS Pro 1400

APC Matrix-UPS 3000

APC Matrix{UPS 3000XR

APC Matrix{UPS 5000*

APC Matrix{UPS 5000XRHardware Compatibility List for Solaris 2.6 (Intel Platform Edition)85

TABLE

1{27

Uninterruptable Power Supplies (UPS)(continued)

APC Smart-UPS 250

APC Smart-UPS 400

APC Smart-UPS 450

APC Smart-UPS 600

APC Smart-UPS 700

APC Smart-UPS 700PM

APC Smart-UPS 700RM

APC Smart-UPS 700XL

APC Smart-UPS 750

APC Smart-UPS 900

APC Smart-UPS 1000

APC Smart-UPS 1000RM

APC Smart-UPS 1000XL

APC Smart-UPS 1250

APC Smart-UPS 1400

APC Smart-UPS 1400RM

APC Smart-UPS 1400RMXL

APC Smart-UPS 1400XLT

APC Smart-UPS 2000

APC Smart-UPS 2200

APC Smart-UPS 2200RM

APC Smart-UPS 2200RMXL

APC Smart-UPS 2200XL

APC Smart-UPS 2200XLT

APC Smart-UPS 3000

APC Smart-UPS 3000RM 86

Hardware

Compatibility List for Solaris 2.6 (Intel Platform Edition)¤ January 1998

TABLE

1{28

Motherboards These are individual motherboards that have been tested as components; see\System

Platforms" on page 7 for a list of tested systems.

Acer M11A (E-IDE PP-200)

Acer M11A (SCSI PP-200)

Acer M9A (1 CPU, PP-166)

Acer M9B (1 CPU, PP-200)

Acer M9B (2 CPUs, PP-200)

Acer X1B (1 CPU, PP-200)

Acer X1B (2 CPUs, PP-200)

AIR 486ET VESA/EISA (Sis chipset)

AIR 54CEP (P-90/100)

AIR 54CDP (2 CPUs, P-90/100)

AIR 54TPI (P-133)

AIR 54TPI (P-200)

AIR P6NPI (PP-200)

AMI Atlas PCI (P-100)

AMI V oyager w/ 486DX2-66 CPU

AMI Super V oyager PCI

AMI Super V oyager II VLB

AMI Titan II (2 CPUs, P-90)

AMI Titan II PCI, EISA (2 CPUs)

AMI Enterprise III w/ 486DX2-66 CPU

AMI Enterprise IVHardware Compatibility List for Solaris 2.6 (Intel Platform Edition)87

TABLE

1{28

Motherboards(continued)

ASUS

C-PKND+P/I P65UP5 (2 CPUs, PII-266)

ASUS HX97 (P-200 MMX)

ASUS KL97-X (PII-266)

ASUS KN97 (PII-233)

ASUS KN97{X (PII-233)

ASUS PCI/E-P54NP4 (2 CPUs, P-90)

ASUS PCI/I-486SP3G (DX33, SX, DX2-66, OverDrives)

ASUS PCI/I-P5SP4 (P-60)

ASUS PCI/I-P54NP4 (2 CPUs, P-90)

ASUS PCI/I-P54NP4D (P-100)

ASUS PCI/I-P54NP4D (P-133)88

Hardware

Compatibility List for Solaris 2.6 (Intel Platform Edition)¤ January 1998

TABLE

1{28

Motherboards(continued)

ASUS, cont.

ASUS

PCI/I-P54SP4 (P-75, 90, 100)

ASUS PCI/I-P54TP4 (P-100)

ASUS PCI/I-P55TP4 (Triton) (P-90)

ASUS PCI/I-P55TP4XE (P-90)

ASUS PCI/I-P55TP4XE (P-133)

ASUS P/E P55T2P4D (2 CPUs, P-133)

ASUS P/E P55T2P4S (P-133)

ASUS P/E P55T2P4S (P-200)

ASUS P/I AP55TV (P-166)

ASUS P/I AP6N (PP-200)

ASUS P/I P55T2P4 (P-200 MMX)

ASUS P/I P55T2P4S (P-133)

ASUS P/I P55T2P4S (P-200)

ASUS P/I P55TVP4 (P-200 MMX)

ASUS P/I P55TXP4 (P-200 MMX)

ASUS P/I P65UP5 (PP-200)

ASUS P/I P65UP5 (2 CPUs, PP-200)

ASUS P/I P6RP4 (PP-150)

ASUS P/I P6RP4 (PP-200)

ASUS P/I XP55T2P4 (P-200 MMX)

ASUS P/I XP55TVP4 (P-200 MMX)

ASUS P/I XP55TXP4 (P-200 MMX)

ASUS P/I XP6NP5 (PP-200)

ASUS P/I XPKNP (PII-233)

ASUS P/I XPKNP5 (PII-233)

ASUS PVI-486AP4 (486SX/DX/DX2)

ASUS PVI-486SP3 (DX33, SX, DX2-66, OverDrives)

ASUS SP97 (AMD K6-200)

ASUS TX97 (P-200 MMX)

ASUS TX97-X (P-200 MMX)

ASUS VL/EISA-486SV1 (DX33, SX, DX2-66, OverDrives)

ASUS VL/I-486SV2G (486SX/DX/DX2)

ASUS VX97 (P-200 MMX)

ASUS VX97-X (P-200 MMX)Hardware Compatibility List for Solaris 2.6 (Intel Platform Edition)89

TABLE

1{28

Motherboards(continued)

DFI G586-VPM (P-90)

DTK FEAT-39 (DX4-100)

DTK PKM0038e

DTK QUIN-54/I (P-133)

FIC PA-2002 (P-75)

FIC PA-2002 (P-100)

FIC PA-2002 (P-133)

FIC PT-2003 (P-75)

FIC PT-2003 (P-120)

FIC PT-2003 (P-150)

FIC PT-2003 (P-166)

GenoaTurbo Express 486VL

GenoaTurbo Express 586 PCI-4

GenoaTurbo Express 586VL

Intel Advanced/AL (Aladdin-Triton) (P-90)

Intel Advanced/AS (Atlantis) (P-166)

Intel Advanced/ATX

Intel Advanced/EV (Endeavor) (P-75)

Intel Advanced/EV (Endeavor) (P-90)

Intel Advanced/EV (Endeavor) (P-100)

Intel Advanced/EV (Endeavor) (P-120)

Intel Advanced/EV (Endeavor) (P-133)

Intel Advanced/EV (Endeavor) (P-150)

Intel Advanced/EV (Endeavor) (P-166)

Intel Advanced/ML (P-133)

Intel Advanced/MN (Morrison) (P-100)90

Hardware

Compatibility List for Solaris 2.6 (Intel Platform Edition)¤ January 1998

TABLE

1{28

Motherboards(continued)

Intel, cont.

Intel

Advanced/PO (P-133)

Intel Advanced/RH (P-133)

Intel Advanced/VS (V enus) (PP-180)

Intel Advanced/ZE Minitower (P-100)

Intel Advanced/ZP (Zappa-Triton) (P-90)

Intel ALTserver (Altair) (P-150)

Intel ALTserver (Altair) (P-166)

Intel ALTserver (Altair) (2 CPUs, P-100)

Intel AN430TX (P-233 MMX)

Intel AP440FX (PP-200)

Intel CN430TX (P-233 MMX)

Intel Express (2 CPUs, P-60)

Intel Express (2 CPUs, P-66)

Intel Express (2 CPUs, P-90)

Intel Xtended Xpress (2 CPUs, P-100)

Intel Xtended Xpress (4 CPUs, P-100)

Intel LT430TX (P-200 MMX)

Intel NP30HX (P-166)

Intel PD440FX (PP-266 MMX)

Intel Performance AU (PP-180)

Intel Performance AU (PP-200)

Intel Premiere/PCI II Baby AT Board (P-90) (sometimes referred to as

Plato) 1

Intel Premiere PCI II (P-100)

Intel RU430HX (P-150)

Intel RU430HX (P-166)

Intel RU430HX (P-233 MMX)

Intel RU430HX 233 MMX (P-233 MMX)

Intel TE430VX (P-166 MMX)

Intel TE430VX (P-200 MMX)

Intel TE430VX (P-233 MMX)

Intel VS440FX (PP-200)

Intel YM430TX (P-233 MMX)Hardware Compatibility List for Solaris 2.6 (Intel Platform Edition)91

TABLE

1{28

Motherboards(continued)

MicronicsEISA 486DX (30, 50, 66 CPU)

Micronics EISA VLB 486DX (30, 50, 66 CPU)

Micronics EISA VLB 486DX2 (30, 50, 66 CPU)

Micronics ISA VLB 486DX2

Micronics JX30 WB (486DX4-100)

Micronics LPH54 (P-75)

Micronics LPH54 (P-90)

Micronics LPH54 (P-100)

Micronics LPH54 (P-120)

Micronics LPH54 (P-133)

Micronics LX30 WB (486SX33)

Micronics M5PE (P-66)

Micronics M5PI (P-66)

Micronics M54HI Plus (P-90)

Micronics M54HI Plus (P-100)

Micronics M54HI Plus (P-120)

Micronics M54HI Plus (P-133)

Micronics M54HI Plus (P-150)

Micronics M54HI Plus (P-166)

Micronics M54HI Triton (P-100)

Micronics M54PE (1 CPU, P-90)

Micronics M54PE (1 CPU, P-100)

Micronics M54PE (1 CPU, P-133)

Micronics M54PE (2 CPUs, P-90)

Micronics M54PE (2 CPUs, P-100)

Micronics M54PE (2 CPUs, P-133)

Micronics M54PI (P-90 or P-75)

Micronics M54SI (P-75)

Micronics M54SI (P-90)

Micronics M54SI (P-100)

Micronics M54LI-1B (P-90)

Micronics M54LI-1B (P-133)

Micronics Mpower 4 plus (486DX2-66)92

Hardware

Compatibility List for Solaris 2.6 (Intel Platform Edition)¤ January 1998

TABLE

1{28

Motherboards(continued)

SuperMicro P55CMS

SuperMicro P5STE (P-133)

SuperMicro P5STE (P-166)

SuperMicro P6DNE (2 CPUs, PP-200)

SuperMicro P6DNF (2 CPUs, PP-200)

Suria SC-4SIO (486DX-Cyrix)

Suria SC-4SIO (486DX2-80-AMD)

Suria SC-4SIO (486DX4-100)

Suria SC-5TIO (P-75)

Suria SC-5TIO (P-133)

Suria SC-5TIO (P-166)

Suria SC-5TIO PB (P-133)

Tulip TC32 (486DX2-66)

Tulip TC40 (486DX2-66)

Tulip TC42 (P-90)

Tulip TC43 (P-90)Hardware Compatibility List for Solaris 2.6 (Intel Platform Edition)93

TABLE

1{28

Motherboards(continued)

Tyan

S1462 (P-120)

Tyan S1462 (P-150)

Tyan S1462 (P-166)

Tyan S1462 (2 CPUs, P-133)

Tyan S1468 (P-120)

Tyan S1470 (P-166)

Tyan S1470 (P-200)

Tyan S1472 ATK (P-166)

Tyan S1472 ATK (P-200)

Tyan S1563D (P-166)

Tyan S1563D (P-200)

Tyan S1563D (2 CPUs, P-166)

Tyan S1563D (2 CPUs, P-200)

Tyan S1662D (PP-200)

Tyan S1668 (2 CPUs, PP-200)

Tyan S1672 (PP-200)

VEGA 486F-3VL with Symphony SL1287, SL82C461, SL82C362 chipset and

486DX2-66 CPU 1.

Only the version that uses Neptune-2 stepping of the PCI chipset has been tested and certi�ed. Note

-Entries marked with an asterisk (*) are newly supported and require

a Driver Update for proper operation. See \How to Obtain Updated

Hardware Compatibility Lists and Device Driver Information" on page 4 for

information about how you can obtain a Driver Update.

Note - \|" in the Bus column indicates a video controller model that is

used on video display adapters and motherboards.

Note - The information in the Video Chip column does not guarantee that

video boards made by another manufacturer using the same chipset will

work. Only the speci�c models listed by V endor, Model, Bus, and Video Chip

have been tested. 94

Hardware

Compatibility List for Solaris 2.6 (Intel Platform Edition)¤ January 1998

TABLE

1{29

Video Display Devices Resolution and Color Depth

800x

600

1024x

768

1152x

900

1280x

1024

1600x

1200

V endor

Model

Bus

Video Chip

8

24

8

24

8

24

8

24

8

24 Acer

ET4000/W32 1

ISA

Tseng

ET4000/W32 X

X

ALR

Flyer

VL

WD90C33

X

AST Manhattan

5090P

2 | Cirrus Logic

GD5424 X

ATI 3D Pro Turbo

PC2TV

* PCI ATI 3D

RAGE II+ X X X X X X X X X 3D

RAGE

3 | ATI 3D RAGE X X X X X

3D RAGE

II 3 | ATI 3D

RAGE II X X X X X X X X X

3D RAGE II+ 3 *

|

ATI 3D

RAGE II+

X

X

X

X

X

X

X

X

X

3D RAGE PRO 3*

|

ATI 3D

RAGE PRO

X

X

X

X

X

X

X

X

X

X

3D Xpression

PCI

ATI 3D RAGE

X

X

X

X

X

3D Xpression+

PC2TV

PCI

ATI 3D

RAGE II

X

X

X

X

X

X

X

X

X

8514 Ultra

ISA

ATI Mach8

X

All-in-Wonder*

PCI

ATI 3D

RAGE II+

X

X

X

X

X

X

X

X

X Graphics

Pro

Turbo

4 PCI ATI Mach64 X X X X X X Hardware

Compatibility List for Solaris 2.6 (Intel Platform Edition)95

TABLE

1{29

Video Display Devices(continued) Resolution and Color Depth

800x

600

1024x

768

1152x

900

1280x

1024

1600x

1200

V endor

Model

Bus

Video Chip

8

24

8

24

8

24

8

24

8

24 Graphics

Pro

Turbo4 VLB ATI Mach64 X X X X X X

Graphics Pro Turbo

1600

PCI

ATI Mach64

X

X

X

X

X

X

X

X

X

Graphics Ultra

ISA

ATI Mach8

X

Graphics Ultra+

ISA

ATI Mach32

X

X

Graphics Ultra Pro

ISA

ATI Mach32

X

X

X

X

Graphics Ultra Pro

PCI

ATI Mach32

X

X

X

X

Graphics Ultra Pro

VLB

ATI Mach32

X

X

X

X Graphics

Xpression

4 PCI ATI Mach64 X X X X X

Graphics

Xpression 4

VLB

ATI Mach64

X

X

X

X

X

Mach64 3

|

ATI Mach64

X

X

Mach64CT 3

|

ATI

Mach64CT

X

X

X

X

X Mach64CT

Rev . 2

3 | ATI

Mach64CT X X X X X

Mach64VT 3

PCI

ATI

Mach64VT

X

X

X

X

X

VGA Wonder+

ISA

ATI Mach8

X

VGA Wonder XL

ISA

ATI Mach8

X 96

Hardware

Compatibility List for Solaris 2.6 (Intel Platform Edition)¤ January 1998

TABLE

1{29

Video Display Devices(continued) Resolution and Color Depth

800x

600

1024x

768

1152x

900

1280x

1024

1600x

1200

V endor

Model

Bus

Video Chip

8

24

8

24

8

24

8

24

8

24 VGA

Wonder XL 24

ISA

ATI Mach8 X

Video Expression

PCI

ATI

Mach64VT

X

X

X

X

X

Winturbo 5

PCI

ATI Mach64

X

X

X

X

X

XPERT@Play *

PCI/

AGP

ATI 3D

RAGE PRO

X

X

X

X

X

X

X

X

X

X

XPERT@Work *

PCI/

AGP

ATI 3D

RAGE PRO

X

X

X

X

X

X

X

X

X

X

Boca

V oyager 64

PCI

S3 Trio64

X

X

X

X

X

Chips &

Technology

65540 3

|

F65540

X

X

65545 3

|

F65545

X

X

X

65548 3

|

F65548

X

X

X

65550 3

|

F65550

X

X

X

X

Cirrus Logic 5420

w/512Kbyte

DRAM

3 | Cirrus Logic

GD5420 X

5428 3

|

Cirrus Logic

GD5428

X

X

X

X 5428

w/512Kbyte

VRAM

3 | Cirrus Logic

GD5428 X

5429 3

|

Cirrus Logic

GD5429

X

X

X

X Hardware

Compatibility List for Solaris 2.6 (Intel Platform Edition)97

TABLE

1{29

Video Display Devices(continued) Resolution and Color Depth

800x

600

1024x

768

1152x

900

1280x

1024

1600x

1200

V endor

Model

Bus

Video Chip

8

24

8

24

8

24

8

24

8

24 5430

3

|

Cirrus Logic

GD5430 X

X

X

X

5434 3

|

Cirrus Logic

GD5434

X

X

X

X

X

X

5436 3

|

Cirrus Logic

GD5436

X

X

X

X

X

54M40 3

|

Cirrus Logic

GD54M40

X

X

X

X

X

5446 3

|

Cirrus Logic

GD5446

X

X

X

X

X

5480 3 *

|

Cirrus Logic

GD5480

X

X

X

X

X

X

X

X

X 7543

chipset

3 | Cirrus Logic

GD7543 X X

Compaq

Professional

Workstation 5000

PCI

MGA 2064W

X

X

X

X

X

X

X

X

X

X

ProLiant

|

Cirrus Logic

GD5420

X

ProLiant 800

|

Cirrus Logic

GD5440

X

ProLiant 1000

|

Cirrus Logic

GD5420

X

ProLiant 1500

|

Cirrus Logic

GD5420

X

ProLiant 2000

|

Cirrus Logic

GD54M30

X 98

Hardware

Compatibility List for Solaris 2.6 (Intel Platform Edition)¤ January 1998

TABLE

1{29

Video Display Devices(continued) Resolution and Color Depth

800x

600

1024x

768

1152x

900

1280x

1024

1600x

1200

V endor

Model

Bus

Video Chip

8

24

8

24

8

24

8

24

8

24 ProLiant

2500

|

Cirrus Logic

GD5420 X

ProLiant 4000

|

Cirrus Logic

GD5420

X

ProLiant 4500

|

Cirrus Logic

GD5424

X

ProLiant 5000

|

Cirrus Logic

GD5424

X

ProLinea

ISA

Tseng ET4000

X

ProSignia 6

|

Cirrus Logic

GD5420

X

ProSignia 300

|

Cirrus Logic

GD5424

X

ProSignia 300/500

|

Cirrus Logic

GD5420

X

ProSignia 300/500

|

Cirrus Logic

GD5424

X

QVision 1024/E

EISA

TRITON

X

QVision 1024/I

ISA

TRITON

X QVision

1280

7 EISA ORION X X X X X

QVision 2000

PCI

Matrox

MGA-2

X

X

X

X

X

QVision 2000 (Rev .

G)

PCI

Matrox

MGA-3

X

X

X

X

X

CompuAdd

Hi-Res VGA

ISA

Tseng ET4000

X Hardware

Compatibility List for Solaris 2.6 (Intel Platform Edition)99

TABLE

1{29

Video Display Devices(continued) Resolution and Color Depth

800x

600

1024x

768

1152x

900

1280x

1024

1600x

1200

V endor

Model

Bus

Video Chip

8

24

8

24

8

24

8

24

8

24 DEC

DECpc XL 590

|

Cirrus Logic

GD5428 X

Dell

DE Series

ISA

Tseng ET4000

X

L Series

|

Tseng

ET4000/W32

X

L Series

|

Tseng

ET4000/W32i

X

M/ME Series

|

S3 805

X

OptiPlex DGX 590

|

ATI Mach64

X

X

X

X

X

OptiPlex XMT 590

|

S3 Vision 864

X

X

X

X

X

PowerEdge SP5xx

|

ATI Mach32

X

Diamond

SpeedStar 24x

ISA

WD90C31

X SpeedStar 64/

SpeedStar 64

Graphics 2000XL

Series ISA/

PCI Cirrus Logic

GD5434 X X X X X

SpeedStar Plus

ISA

Tseng ET4000

X

SpeedStar Pro/

SpeedStar Pro 1100

ISA

Cirrus Logic

GD5426

X

Stealth 3D 2000

PCI

S3 ViRGE

(86C325)

X

X

X

X

X Stealth 3D

2000/Pro* PCI S3 ViRGE/DX

(86C375) X X X X X X

Stealth 3D 3000

PCI

S3 ViRGE/VX

(86C988)

X

X

X

X

X

X

X

X

X 100

Hardware

Compatibility List for Solaris 2.6 (Intel Platform Edition)¤ January 1998

TABLE

1{29

Video Display Devices(continued) Resolution and Color Depth

800x

600

1024x

768

1152x

900

1280x

1024

1600x

1200

V endor

Model

Bus

Video Chip

8

24

8

24

8

24

8

24

8

24 Stealth 24

ISA

S3 801 X

Stealth 32

PCI

Tseng

ET4000/W32p

X

X

X

X

X

Stealth 32

VLB

Tseng

ET4000/W32p

X

X

X

X

X Stealth 64 DRAM/

Stealth 64 Graphics

2000 Series PCI/

VLB S3 Vision 864 X X X X X

Stealth 64 DRAM

PCI

S3 Trio64

X

X

X

X

X

Stealth 64 VRAM

PCI

S3 Vision 964

X

X

X

X

X

X

X

Stealth 64 VRAM

VLB

S3 Vision 964

X

X

X

X

X

X

X Stealth Video

DRAM/ Stealth 64

Video 2000 Series PCI/

VLB S3 Vision 868 X X X X X X

Stealth 64 Video

2001

PCI

S3 Vision 765

X

X

X

X

X Stealth Video

VRAM/ Stealth 64

Video 30008 Series PCI S3 Vision 968 X X X X X X X X X

Stealth Pro

ISA

S3 928

X

X

X

X

Stealth SE

PCI

S3 Trio32

X

X

X

Stealth VRAM

ISA

S3 911

X

Viper PCI

PCI

Weitek Power

9000

X

X

X

X

Viper VLB

VLB

Weitek Power

9000

X

X

X

X Hardware

Compatibility List for Solaris 2.6 (Intel Platform Edition)101

TABLE

1{29

Video Display Devices(continued) Resolution and Color Depth

800x

600

1024x

768

1152x

900

1280x

1024

1600x

1200

V endor

Model

Bus

Video Chip

8

24

8

24

8

24

8

24

8

24 Viper Pro

PCI

Weitek Power

9100 X

X

X

X

Viper Pro

VLB

Weitek Power

9100

X

X

X

X

Viper SE9

PCI

Weitek Power

9100

X

X

X

X

ELSA

Victory 3D

PCI

S3 ViRGE

(86C325)

X

X

X

X

X

X

Winner 1000

VLB

S3 928

X

X

X

Winner 1000 A VI

PCI

S3 Vision 868

X

X

X

X

X

Winner 2000

VLB

S3 928

X

X

X

X Winner

1000Pro-

VL 10 VLB S3 Vision 864 X X X X X

Winner

2000Pro-PCI

PCI

S3 Vision 964

X

X

X

X

X

X

X

X

Winner 2000Pro-VL

VLB

S3 Vision 964

X

X

X

X

X

X

X

X

Winner 2000Pro-X

PCI

S3 Vision 968

X

X

X

X

X

X

X

X

X

Winner 3000-S

PCI

S3 ViRGE

(86C325)

X

X

X

X

X

Everex

FIC 864P

PCI

S3 Vision 864

X

X

X

X

X

VGA Trio 64P

PCI

S3 Trio64

X

X

X

X

X

ViewPoint 64P

PCI

S3 Vision 864

X

X

X

X

X

Genoa

SuperVGA 7000

X 102

Hardware

Compatibility List for Solaris 2.6 (Intel Platform Edition)¤ January 1998

TABLE

1{29

Video Display Devices(continued) Resolution and Color Depth

800x

600

1024x

768

1152x

900

1280x

1024

1600x

1200

V endor

Model

Bus

Video Chip

8

24

8

24

8

24

8

24

8

24 Hercules

Dynamite

128/Video

PCI

Tseng ET6000 X

X

X

X

X

X

Hewlett-

Packard

HP NetServer

LC/LE/LF

TVGA 9000i

X

HP V ectra VL2

Cirrus Logic

GD5428

X

X

HP V ectra XM2i

S3 Vision 864

X

X

X HP V ectra

XU11 | S3 Vision 864 X X X X X

IBM Easy

Options

(VC550)

12 ISA Cirrus Logic

GD5428 X

PC 330|Model

6575

|

S3 Vision 864

X

X

X

X

X

PC 330|Model

6576

|

S3 Trio64

X

X

X

PC 350|Model

6581

|

Cirrus Logic

GD5430

X

X

X

X

PC 360|Model

6598

|

MGA Storm

X

X

X

X

X

X

X

X

PC 750|Model

6885-35H

|

S3 Vision 864

X

X

X

X

X

PC 750|Model

6885-J0M

|

S3 Vision 864

X

X

X

X

X

PC Series 300-486

|

Cirrus Logic

GD5430

X

X

PC Series 300

|

S3 Vision 864

X

X

X

X

X Hardware

Compatibility List for Solaris 2.6 (Intel Platform Edition)103

TABLE

1{29

Video Display Devices(continued) Resolution and Color Depth

800x

600

1024x

768

1152x

900

1280x

1024

1600x

1200

V endor

Model

Bus

Video Chip

8

24

8

24

8

24

8

24

8

24 PC

Series 700

|

S3 Vision 864 X

X

X

X

X PC Server

310|Model

8639-0DT | S3 Vision 868 X X X X

PC Server

310|Model

8639-0EO | S3 Trio64V+ X X X

PC Server

310|Model

8639-0XT | S3 Vision 864 X X X

PC Server

320|Model

8640-0DV | Cirrus Logic

GD5428 X X

PC Server

320|Model

8640-0NJ | Cirrus Logic

GD5428 X X

PC Server

320|Model

8640-0XT | Cirrus Logic

GD5428 X X

PC Server

320|Model

8640-0YT | Cirrus Logic

GD5428 X X

PC Server

320|Model

8640-MXT | Cirrus Logic

GD5430 X X

PC Server

325|Model

8639-ESO | Cirrus Logic

GD5436 X X X

PC Server

325|Model

8639-ESV | Cirrus Logic

GD5436 X X X 104

Hardware

Compatibility List for Solaris 2.6 (Intel Platform Edition)¤ January 1998

TABLE

1{29

Video Display Devices(continued) Resolution and Color Depth

800x

600

1024x

768

1152x

900

1280x

1024

1600x

1200

V endor

Model

Bus

Video Chip

8

24

8

24

8

24

8

24

8

24 PC

Server

500|Model

8641-0YR | Cirrus Logic

GD5428 X X

PC Server

500|Model

8641-0YT | Cirrus Logic

GD5428 X X

PC Server

520|Model

8641-ED2 | Cirrus Logic

GD5428 X X

PC Server

520|Model

8641-EDG | Cirrus Logic

GD5428 X X

PC Server

520|Model

8641-EZS | Cirrus Logic

GD5428 X X

PC Server

520|Model

8641-EZV | Cirrus Logic

GD5428 X X

PC Server

720|Model

8642-0ZO | Cirrus Logic

GD5428 X X

PS/ValuePoint

|

S3 805

X

PS/ValuePoint

Performance Series

|

S3 Vision 864

X

X

X

X

X

VGA 13

ISA

IBM VGA

X

XGA

MCA

XGA

X

X

XGA-2

MCA

XGA-2

X

Intel

Professional/GX

High Resolution

|

ATI Mach32

X

X

X

X Hardware

Compatibility List for Solaris 2.6 (Intel Platform Edition)105

TABLE

1{29

Video Display Devices(continued) Resolution and Color Depth

800x

600

1024x

768

1152x

900

1280x

1024

1600x

1200

V endor

Model

Bus

Video Chip

8

24

8

24

8

24

8

24

8

24 TMI/IPG

|

WD9031A X

Xpress VGA

|

WD90C31

X

Intergraph

TD-1 14

|

S3 928

X

X

X

X TD-2,

TD-3;

(G90)

15 PCI Weitek Power

9000 X X X X

G91 16

PCI

Weitek Power

9100

X

X

X

G95 17

PCI

MGA Storm

X

X

X

X

X

X

X

X

X

X ISMP

(SMP

224)

18 Cirrus Logic

GD5434 X X X X X X

Matrox

MGA Impression

VLB

Matrox

MGA-1

X

X

X

X

X

X

X

MGA Impression

Plus

PCI

Matrox

MGA-3

X

X

X

X

MGA Ultima

VLB

Matrox

MGA-2

X

X

X

X

X

MGA Ultima Plus

PCI

Matrox

MGA-2

X

X

X

X

X

X

MGA Ultima Plus

200

PCI

Matrox

MGA-2

X

X

X

X

X

X

X

X

Millennium

PCI

MGA

Storm-R1

X

X

X

X

X

X

X

X

X

X

Millennium 220

PCI

MGA

Storm-R2

X

X

X

X

X

X

X

X

X

X 106

Hardware

Compatibility List for Solaris 2.6 (Intel Platform Edition)¤ January 1998

TABLE

1{29

Video Display Devices(continued) Resolution and Color Depth

800x

600

1024x

768

1152x

900

1280x

1024

1600x

1200

V endor

Model

Bus

Video Chip

8

24

8

24

8

24

8

24

8

24 Millennium 220

PCI

MGA2064{R2 X

X

X

X

X

X

X

X

X

X

Millennium 220*

PCI

MGA2064W{

R3

X

X

X

X

X

X

X

X

X

X

Millennium II*

PCI/

AGP

MGA 2164W

X

X

X

X

X

X

X

X

X

X

Mystique

PCI

MGA 1064SG

X

X

X

X

X

X

X

X

X

Mystique 220*

PCI

MGA1064SG

(-G or -H)

X

X

X

X

X

X

X

X

X

Micronics Mpower 4

plus

4 | ATI Mach64 X X

Miro miroCRYSTAL

20SD

PCI

S3 Vision 864

X

X

X

X

X miroCRYSTAL

40SV

PCI

S3 Vision 964

X

X

X

X

X

X

X miroMagic

ISA

S3 805

X

X

Nanao

EizoAccel AA51

ISA

CHIPS

F82C480

X

X

Nanao HA50/HL50

ISA

S3 928

X

X

X

Nanao HA60

ISA

S3 928

X

X

X

Number Nine

#9GXE 19

ISA

S3 928

X

X

X

X

#9GXE 19

VLB

S3 928

X

X

X

X

#9GXE64

PCI

S3 Vision 864

X

X

X

X

X

X

#9GXE64 Pro

PCI

S3 Vision 964

X

X

X

X

X

X

X

X Hardware

Compatibility List for Solaris 2.6 (Intel Platform Edition)107

TABLE

1{29

Video Display Devices(continued) Resolution and Color Depth

800x

600

1024x

768

1152x

900

1280x

1024

1600x

1200

V endor

Model

Bus

Video Chip

8

24

8

24

8

24

8

24

8

24 9FX

Motion 331

PCI

S3 Trio64V+ X

X

X

X

X

9FX Motion 531

PCI

S3 Vision 868

X

X

X

X

9FX Motion 771

PCI

S3 Vision 968

X

X

X

X

X

X

X

X

X

9FX Reality 332

PCI

S3 ViRGE

(86C325)

X

X

X

X

X

Imagine 128

PCI

Imagine 128

X

X

X

X

X

X

X

X

Imagine 128 Pro

PCI

Imagine 128

X

X

X

X

X

X

X

X

X

X

Imagine 128 Series

2

PCI

Imagine 128

V2

X

X

X

X

X

X

X

X

Imagine 128 Series

2e

PCI

Imagine 128

V2

X

X

X

X

X

X

X

Vision330 20

PCI

S3 Trio64

X

X

X

X

X

Oak

Technology

OTI107

PCI

OTI107

X

X

X

X

X

OTI111

PCI

OTI111

X

X

X

X

X

Orchid

Fahrenheit 1280

ISA

S3 924

X

Fahrenheit 1280

Plus

ISA

S3 801

X

Fahrenheit 1280

Plus

VLB

S3 801

X

X

Fahrenheit V A

ISA

S3 801

X

Kelvin 64

PCI

Cirrus Logic

GD5434

X

X

X

X

X 108

Hardware

Compatibility List for Solaris 2.6 (Intel Platform Edition)¤ January 1998

TABLE

1{29

Video Display Devices(continued) Resolution and Color Depth

800x

600

1024x

768

1152x

900

1280x

1024

1600x

1200

V endor

Model

Bus

Video Chip

8

24

8

24

8

24

8

24

8

24 Kelvin

6421 VLB Cirrus Logic

GD5434 X X X X X

Prodesigner IIs

ISA

Tseng ET4000

X

S3

928 3

|

S3 938

X

X

X

X

Trio32 3

|

S3 Trio32

X

X

Trio64 3

|

S3 Trio64

X

X

X

X

X

Trio64V+ 3

|

S3 Trio64V+

X

X

X

X

X Trio64V2/DX

3 | S3

Trio64V2/DX

(86C755) X X X X X

ViRGE 3

|

S3 ViRGE

(86C325)

X

X

X

X

X

X

ViRGE/DX 3*

PCI

S3 ViRGE/DX

(86C375)

X

X

X

X

X

X

ViRGE/GX 3*

PCI

S3 ViRGE/GX

(86C385)

X

X

X

X

X

X

X

ViRGE/VX 3

|

S3 ViRGE/VX

(86C988)

X

X

X

X

X

X

X

X

X Vision

864 3 S3 Vision 864 X X X X X

Vision

868 3 | S3 Vision 868 X X X X

SPEA

V7-Mercury

ISA

X Hardware

Compatibility List for Solaris 2.6 (Intel Platform Edition)109

TABLE

1{29

Video Display Devices(continued) Resolution and Color Depth

800x

600

1024x

768

1152x

900

1280x

1024

1600x

1200

V endor

Model

Bus

Video Chip

8

24

8

24

8

24

8

24

8

24 V7-Mirage

P-64

PCI

S3 Vision 868 X

X

X

X

X

STB

Lightspeed 128

PCI

Tseng ET6000

X

X

X

X

X

Lightspeed VL

VLB

Tseng

ET4000/W32p

X

X

X

X

X

Nitro 3D*

PCI

S3 ViRGE/GX

(86C385)

X

X

X

X

X

X

X

Nitro 64 Video*

PCI

Cirrus Logic

GD5446

X

X

X

X

X

Nitro PCI

PCI

Cirrus Logic

GD5434

X

X

X

X

X

X

PowerGraph 64

PCI

S3 Trio64

X

X

X

X

X

PowerGraph 64 3D*

PCI

S3 ViRGE

(86C325)

X

X

X

X

X

X

PowerGraph 64

Video

PCI

S3 Trio64V+

X

X

X

X

X

PowerGraph ERGO

ISA

Tseng ET4000

X

PowerGraph PRO

PCI

PCI

S3 Vision 864

X

X

X

X

X

V elocity 3D

PCI

S3 ViRGE/VX

(86C988)

X

X

X

X

X

X

X

X

X

V elocity 64V

PCI

S3 Vision 968

X

X

X

X

X

X

X

X

Toshiba J3100 | Western

Digital

90C31A X X

Trident

9440 22

PCI

TGUI9440

X

X

9680

PCI

TGUI9680

X

X

X

X 110

Hardware

Compatibility List for Solaris 2.6 (Intel Platform Edition)¤ January 1998

TABLE

1{29

Video Display Devices(continued) Resolution and Color Depth

800x

600

1024x

768

1152x

900

1280x

1024

1600x

1200

V endor

Model

Bus

Video Chip

8

24

8

24

8

24

8

24

8

24 9685

PCI

TGUI9685 X

X

X

X

TVGA 8900C

ISA

Trident 8900C

X

TVGA 9000i

ISA

Trident 9000i

X

Tseng

Tseng ET6000

|

Tseng ET6000

X

X

X

X

X

Western

Digital

Paradise

Accelerator

ISA

WD90C31

X 1.

The ET4000/W32 video cards that are shipped with Acer machines are not all the same. If you encounter any display

problems when the window system is running, try using a different add-on board that is compatible with the Solaris

operating environment.

2. Video adapters based on the Cirrus Logic GD5424 chipset with 512-Kbyte DRAM may not perform well in 800x600x256

mode, particularly if the selected monitor refresh rate is 60 Hz or higher.

3. SunSoft does not guarantee that every video card with this video chip will work, but it is possible that your model will be

one of a large number that can be used successfully.

4. Support is provided for ATI cards with ATI Mach64 chips and these RAMDACS: ATT68860, ATT20C408, ATT20C491,

ATT20C498, STG1702, and STG1703.

5. The ATI Winturbo model is equivalent to the Gateway ATI GX Mach64 PCI video card.

6. The ProSignia 300 systems and some models of the ProSignia Server systems with the Cirrus Logic 5424 graphics chip are

supported. Choose one of the \Cirrus Logic 5424 (512k)" entries when con�guring the window system usingkdmconfig.

7. Used on the Compaq QVision 1280/E Graphics Controller and in the Compaq Deskpro 590.

8. For cards using the IBM or TI RAMDACs only.

9. The Diamond Viper SE is not supported at 80 Hz in 1280x1024 resolution.

10. The ELSA Winner 1000Pro with the ATT20C498 RAMDAC is supported.

11. Both the STG1702 and the ATT21C498 RAMDACs are supported.

12. Select \Cirrus Logic 542x" when con�guring the display adapter during Solaris installation.

13. 640x480, 16 colors. Any 256-Kbyte or better VGA adapter supporting standard IBM mode 0x12 graphics. For VGA with

800x600 virtual screen, select \16 color, 640x480 VGA panning @800x600 (for experts only, see docs)" when con�guring the

display adapter during Solaris installation. Warning: This selection enables panning mode on a standard VGA. This video

mode supports a virtual resolution of 800x600, but is only capable of physically displaying 640x480 pixels at a time. This

may be a preferred mode to use on small screens, but the use of panning may require some training. For more

information, see the documentation supplied with Video Driver Updates for Solaris 2.6 Intel Platform Edition, available on

the Web at http://access1.sun.com/drivers/.

14. To support 1152x900 or 1280x1024 resolution on the Intergraph TD-1 display adapter, you must select an interlaced

monitor type when con�guring the Solaris window system. Choose \Multifrequency 56kHz (up to 1280x1024 interlaced)"

as the monitor type. See the documentation supplied with Video Driver Updates for Solaris 2.6 Intel Platform Edition,

available on the Web at http://access1.sun.com/drivers/ for more information.

15. The Intergraph G90 is synonymous with the Diamond Viper video card.

16. The Intergraph G91 also supports a resolution of 1600x1280 for 8-bit color. For additional information on this model, see

the Device Reference Page.

17. To support the Intergraph G95, select the graphics card \Matrox MGA Millennium" when con�guring the Solaris window

system.

18. To support the Intergraph ISMP , select the graphics card \Cirrus Logic GD5434" when con�guring the Solaris window

system.

19. The Number Nine #9GXE video display adapters (ISA and VESA local bus) support 24-bit color in 640x480 mode only.Hardware

Compatibility List for Solaris 2.6 (Intel Platform Edition)111

TABLE

1{29

Video Display Devices(continued)

20. Select \#9GXE 64 (Trio64)" when con�guring the display adapter during Solaris installation.

21. Older versions of the Orchid Kelvin 64 VLB card have memory addressing limitations that may cause problems if your

system contains 32 Mbytes or more of RAM. For more information, see the documentation supplied with Video Driver

Updates for Solaris 2.6 Intel Platform Edition, available on the Web athttp://access1.sun.com/drivers/.

22. This card does not work at the 1024x768 resolution with a 56-kHz refresh rate. Note

-For a list of Notebook Computers that have been tested with the

Solaris 2.6Intel Platform Edition operating environment, see T able 1{3.

Note - Entries marked with an asterisk (*) are newly supported and require

a Video Driver Update for proper operation.

TABLE 1{30 Notebook Display Video Support Resolution and Color Depth

E=With External Monitor

I=With Internal Monitor

640x480

800x600

1024x768

1280x1024

V endor

Model

Video Chip

8

24

8

24

8

24

8

24 Ambra

SN425C 1

WD 90C24

I

AST

Ascentia 950N

w/SVGA Panel

Cirrus Logic

GD7543

E,I

E,I

E

PowerExec

4/33SL

WD 90C26

I

Chips &

Technology 65550

2 Chips &

Technology

65550 E,I E,I E, I

Compaq

ARMADA 4120T

Cirrus Logic

GD7548

E,I

E

LTE 4/25C

WD 90C24

I

LTE 4/33C

WD 90C24

I

LTE Elite 4/40C

WD 90C24

E,I

E

E 112

Hardware

Compatibility List for Solaris 2.6 (Intel Platform Edition)¤ January 1998

TABLE

1{30

Notebook Display Video Support(continued) Resolution and Color Depth

E=With External Monitor

I=With Internal Monitor

640x480

800x600

1024x768

1280x1024

V endor

Model

Video Chip

8

24

8

24

8

24

8

24 LTE

5100

Cirrus Logic

GD7543

E,I

E,I

E

LTE 5200

Cirrus Logic

GD7543

E,I

E,I

E

Dell

Latitude LM

P133ST

NeoMagic

NM2070

E,I

E

Latitude XPi 75D

Cirrus Logic

GD7543

E,I

E

E

Latitude XPi CD

NeoMagic

NM2090

E,I

E

Latitude XPi

P133ST

NeoMagic

NM2070

E,I

E

Ergo

Power Brick

WD 90C24

I

HP Omni 5550 Chips &

Technology

65548 E,I E,I E

IBM ThinkPad

365XD

3 Trident 9320 E,I E

ThinkPad 750

WD 90C24

E,I

ThinkPad 750C

WD 90C24

I

ThinkPad 755C

WD 90C24

E,I

E

E

ThinkPad 755CD

WD 90C24

E,I

E

E

ThinkPad 755CV

WD 90C24

E,I

E

E

ThinkPad 755CX

w/SVGA Panel

WD 90C24

E,I

E,I

E Hardware

Compatibility List for Solaris 2.6 (Intel Platform Edition)113

TABLE

1{30

Notebook Display Video Support(continued) Resolution and Color Depth

E=With External Monitor

I=With Internal Monitor

640x480

800x600

1024x768

1280x1024

V endor

Model

Video Chip

8

24

8

24

8

24

8

24 ThinkPad

760CD

Trident 9320

E,I

E

ThinkPad 760ED

Trident 9385

E,I

E

E

ThinkPad 760ED

w/XVGA

Trident 9385

E,I

E

ThinkPad 760EL

Trident 9385

E,I

E

NEC

V ersa/50

WD 90C24

I V ersa M75C Chips &

Technology

65540 E,I E E

V ersa M75HC Chips &

Technology

65545 E,I E,I E

V ersa UltraLite

WD 90C24

I

Panasonic

CF-V211 1

WD 90C24

I

TI

Extensa 560CDT

Cirrus Logic

GD7543

E,I

E

E

TravelMate

4000E TFT

Cirrus Logic

GD6440

I

Toshiba

4800CT

WD 90C24

E,I

E

E

4850CT

WD 90C24

E,I

E

E 4900CT Chips &

Technology

65545 E,I E E 114

Hardware

Compatibility List for Solaris 2.6 (Intel Platform Edition)¤ January 1998

TABLE

1{30

Notebook Display Video Support(continued) Resolution and Color Depth

E=With External Monitor

I=With Internal Monitor

640x480

800x600

1024x768

1280x1024

V endor

Model

Video Chip

8

24

8

24

8

24

8

24 Portege

610CT Chips &

Technology

65546 E,I E E

Portege 650CT Chips &

Technology

65550 E,I E E

Portege 660CDT Chips &

Technology

65554 E,I E E

Satellite

200CDS* Chips &

Technology

65550 E,I E E

Satellite

220CDS* Chips &

Technology

65554 E,I E E

Satellite Pro

400CDT Chips &

Technology

65546 E,I E E

Satellite Pro

410CDT Chips &

Technology

65548 E,I E,I E

Satellite Pro

425CDT Chips &

Technology

65550 E,I E,I E E

T3400

WD 90C24

I

T4400C

WD 90C30

I

T4600C

WD 90C26

I

T4700C

WD 90C24

I Hardware

Compatibility List for Solaris 2.6 (Intel Platform Edition)115

TABLE

1{30

Notebook Display Video Support(continued) Resolution and Color Depth

E=With External Monitor

I=With Internal Monitor

640x480

800x600

1024x768

1280x1024

V endor

Model

Video Chip

8

24

8

24

8

24

8

24 Tecra

500CDT Chips &

Technology

65550 E,I E,I E E

Tecra 520CDT Chips &

Technology

65555 E,I E E

Tecra 530CDT* Chips &

Technology

65555 E,I E

Tecra 720CDT Chips &

Technology

65550 E,I E,I E,I E

Tecra 730CDT Chips &

Technology

65550 E,I E,I E,I E

Tecra

740CDT

3 Chips &

Technology

65554 E,I E

Tecra 700CT Chips &

Technology

65548 E,I E,I E

Twinhead

Slimnote 486E

WD 90C24

I

Zenith

Data

Systems Z-Note GT Chips &

Technology

65548 E,I E,I E

Z-Note ex

WD 90C24

E,I

E

E 1. Select \T3400ct,T4700ct, Twinhead 486E, ThinkPad 750: WD90C24 w/1Mb" when con�guring the display adapter during

Solaris installation.

2. Both SVGA and XGA panels are supported.

3. Not tested by SunSoft, but reported to work. Panning is not supported for this notebook.116

Hardware

Compatibility List for Solaris 2.6 (Intel Platform Edition)¤ January 1998